{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["原材料","新阳1-6月采购备品备件","同集1-6月采购备品备件"],"read":"whole","date_system":"1900"}

{"sheet":"原材料","index":0,"n_rows":11,"n_cols":3,"rows_kept":11,"merged":[[1,0,2,0],[1,1,1,2],[10,0,10,2]]}
[]
["名称","年采购量（吨）"]
[null,"新阳热电","同集热电"]
["煤炭","10-12万","5-6万"]
["消石灰",4000,2000]
["石灰石",4000,2000]
["盐酸",300,150]
["烧碱",300,150]
["液氧",1000,500]
["氨水",400,60]
["备注：以上数量为2022年采购大概量，每年采购量根据供热负荷有所变化。"]

{"sheet":"新阳1-6月采购备品备件","index":1,"n_rows":555,"n_cols":10,"rows_kept":555,"merged":[[0,0,0,9],[1,0,1,9],[7,9,8,9],[22,3,23,3],[22,9,23,9],[33,9,34,9],[35,9,36,9],[38,1,40,1],[48,1,49,1],[48,9,49,9],[50,9,53,9],[73,1,77,1],[73,9,77,9],[78,1,79,1],[82,1,90,1],[85,9,90,9],[95,9,96,9],[98,9,101,9],[106,8,108,8],[106,9,108,9],[109,1,110,1],[109,8,115,8],[111,1,112,1],[113,1,115,1],[124,1,125,1],[144,9,145,9],[153,9,154,9],[154,3,155,3],[158,1,170,1],[158,3,170,3],[171,1,172,1],[171,3,172,3],[173,8,174,8],[180,1,184,1],[180,8,184,8],[180,9,192,9],[185,1,190,1],[191,1,192,1],[195,8,198,8],[195,9,198,9],[199,9,200,9],[201,1,203,1],[201,9,203,9],[205,9,206,9],[209,1,210,1],[209,9,212,9],[211,1,212,1],[215,1,216,1],[215,9,216,9],[217,1,218,1],[217,9,218,9],[219,1,224,1],[219,9,226,9],[225,1,226,1],[228,1,229,1],[232,1,233,1],[232,3,233,3],[232,8,233,8],[234,1,235,1],[234,9,237,9],[236,1,237,1],[239,1,240,1],[278,8,279,8],[278,9,279,9],[284,8,288,8],[285,9,288,9],[300,8,301,8],[302,8,303,8],[302,9,303,9],[316,9,317,9],[348,1,356,1],[372,9,373,9],[378,8,379,8],[386,9,387,9],[390,9,391,9],[393,9,394,9],[395,0,395,9],[411,0,411,9],[418,8,419,8],[418,9,419,9],[421,8,423,8],[421,9,423,9],[428,1,432,1],[428,8,432,8],[428,9,432,9],[444,8,446,8],[447,0,447,9],[449,8,452,8],[455,0,455,9],[472,0,472,9],[474,1,476,1],[484,1,485,1],[489,1,490,1],[495,1,496,1],[495,8,496,8],[497,1,498,1],[497,8,498,8],[504,0,504,9],[525,0,525,9],[531,1,538,1],[539,1,540,1],[541,9,543,9],[546,1,548,1],[549,0,549,9]]}
["2023年1月~6月备品备件采购"]
["五金配件、管材类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"PVC弯头","45°PVC弯头  φ325","PVC","个",1]
[2,"PVC弯头","ø110  ","PVC-U","个",1,{"$nulls":3},"雨水井改造"]
[3,"PVC法兰","ø110  ","PVC-U","个",1,{"$nulls":3},"雨水井改造"]
[4,"PVC管","ø110  PVC-U","PVC-U","米",1,{"$nulls":3},"雨水井改造"]
[5,"PVC45°弯头","ø20","PVC-U","个",1,{"$nulls":3},"0米层空调排水管改造"]
[6,"PVC三通","ø20","PVC-U","个",1]
[7,"PVC线槽","阻燃绝缘 24*14   4米",null,"条",1,null,null,"联塑","耗品"]
[8,"PVC线管","绝缘阻燃电工套管 DN20*1.8   4米",null,"条",1,null,null,"联塑","耗品"]
[9,"PVC线管","绝缘阻燃电工套管 DN25*2.0   4米",null,"条",1,null,null,"联塑","耗品"]
[10,"PVC线管直通","DN20",null,"只",1,null,null,"联塑","耗品"]
[11,"PVC线管鞍型管卡","DN20",null,"只",1,null,null,"联塑","耗品"]
[12,"PVC线管90度弯头","DN20",null,"只",1,null,null,"联塑","耗品"]
[13,"PVC线管三通","DN20",null,"只",1,null,null,"联塑","耗品"]
[14,"PVC胶水","500ml",null,"瓶",1,{"$nulls":3},"雨水井改造"]
[15,"UPVC法兰球阀","DN50","UPVC","个",1,{"$nulls":3},"化水酸罐用"]
[16,"UPVC法兰","ø63","UPVC","个",1,{"$nulls":3},"化水酸罐用"]
[17,"UPVC弯头","ø63","UPVC","个",1,{"$nulls":3},"化水酸罐用"]
[18,"UPVC管","ø63","UPVC","米",1,{"$nulls":3},"化水酸罐用"]
[19,"UPVC直接","ø63","UPVC","个",1,{"$nulls":3},"排污井用"]
[20,"弯头","90°φ159*5","碳钢GB/8163-2008","个",1,{"$nulls":3},"化水高效更换用"]
[21,"无缝钢管","φ159*5 （单根约12米）",null,"米",1]
[22,"钢管","Φ108×6 20G需附有特种设备生产许可证无缝钢管生产B级及以上资质”、材料必须是原厂家出厂并提供相应证明材料及出厂技术标准且符合需方使用等技术要求。","20G GB/5310-2007","米",1,{"$nulls":3},"锅炉给水管"]
[23,"钢管","Φ57×3.5 20G需附有特种设备生产许可证无缝钢管生产B级及以上资质”、材料必须是原厂家出厂并提供相应证明材料及出厂技术标准且符合需方使用等技术要求。","20G GB/5310-2007","米",1,{"$nulls":3},"锅炉减温水管"]
[24,"钢管","Φ57×5  20G需附有特种设备生产许可证无缝钢管生产B级及以上资质”、材料必须是原厂家出厂并提供相应证明材料及出厂技术标准且符合需方使用等技术要求。","20G GB/5310-2007","米",1,{"$nulls":3},"锅炉再循环管"]
[25,"弯头90°","Φ108×6  20G","20G GB/5310-2007","个",1,{"$nulls":3},"锅炉给水管"]
[26,"弯头90°","Φ57×3.5  20G","20G GB/5310-2007","个",1,{"$nulls":3},"锅炉减温水管"]
[27,"弯头90°","Φ57×5  20G","20G GB/5310-2007","个",1,{"$nulls":3},"锅炉再循环管"]
[28,"三通接头","DN32","碳钢","个",1,{"$nulls":3},"空压机冷却水改造"]
[29,"弯头90°","ø110*5mm   1.5D","碳钢","个",1]
[30,"弯头90°","159*4.5mm","Q235B","个",1,{"$nulls":3},"1#炉回料改造"]
[31,"等径三通","DN250  壁厚5mm","不锈钢","个",1,{"$nulls":3},"工业冷却水回水至循环水池应急排放"]
[32,"90°热压无缝弯头"," R=1.0D  DN250  壁厚5mm","不锈钢","个",1]
[33,"等径三通","DN150  壁厚5mm","碳钢","个",1,{"$nulls":3},"臭氧系统冷却水回水至循环水池应急排放"]
[34,"90°热压无缝弯头","R=1.0D  DN150  壁厚5mm","碳钢","个",1]
[35,"大小头","DN40化DN25  PN25",8163,"个",1,{"$nulls":3},"外管流量计缩径改造用"]
[36,"异径接头     （大小头）","DN100-DN65  5mm","碳钢","个",1,{"$nulls":3},"雨水井改造"]
[37,null,"DN159-DN100  5mm","碳钢","个",1,{"$nulls":3},"雨水井改造"]
[38,null,"DN125-DN100  5mm","碳钢","个",1,{"$nulls":3},"雨水井改造"]
[39,"镀锌管","DN32*3mm",null,"米",1,{"$nulls":3},"日常耗材"]
[40,"不锈钢管","DN25*3mm",304,"米",1,{"$nulls":3},"日常耗材"]
[41,"镀锌管","ø110*4mm","镀锌","米",1,{"$nulls":3},"雨水井改造"]
[42,"镀锌管","1.5寸*3.5mm","镀锌管","米",1]
[43,"镀锌角钢","L40*4mm",null,"根",1,{"$nulls":3},"日常耗材"]
[44,"镀锌角钢","L50*5mm",null,"根",1,{"$nulls":3},"日常耗材"]
[45,"镀锌角钢","50*50*4mm",null,"米",1,{"$nulls":3},"耗品"]
[46,"不锈钢弯头90°","ø32*3.5mm",304,"个",1,{"$nulls":3},"日常耗品配件"]
[47,null,"ø38*3.5mm",304,"个",1]
[48,"焊接大小头","304不锈钢 57*48*3.0","310S","个",1,{"$nulls":3},"汽化器改造"]
[49,"焊接弯头","304不锈钢 51*3.0","310S","个",1]
[50,"法兰","304不锈钢 DN50 PN25","310S","片",1]
[51,"法兰","304不锈钢 DN50 PN16","310S","片",1]
[52,"法兰盘","DN100 1.6mpa","碳钢","个",1,{"$nulls":3},"雨水井改造"]
[53,"法兰","DN150  1.6mpa","Q235B","片",1,{"$nulls":3},"1#炉回料改造"]
[54,"钢丝绳卡","M20","镀锌锰钢","个",1,{"$nulls":3},"干煤棚行车用"]
[55,"限高警示牌","φ600mm （4米）","铝","个",1,{"$nulls":3},"干煤棚大门用"]
[56,"限高牌","直径60、（内容5M）含抱箍",null,"片",1,{"$nulls":3},"外管更换"]
[57,"多功能梯","MDL-410D  伸缩梯子多功能人字梯",null,"只",1,null,null,"镁多力（midoli）","登高作业"]
[58,"硬胶套","A4透明PVC,35丝横开半圆口",null,"个",1,{"$nulls":3},"安全整改用"]
[59,"3M强力双面胶","1.5cm*33m 厚度0.8mmVHB防水无痕高粘度",null,"卷",1,{"$nulls":3},"安全整改用"]
[60,"高压软管","  DN38 1.5米 1.0MPa 带活接头",null,"条",1,{"$nulls":3},"空压机冷却水改造"]
[61,"内接头","DN32","碳钢","个",1,{"$nulls":3},"空压机冷却水改造"]
[62,"双丝接头","DN32","镀锌","个",1,{"$nulls":3},"空压机冷却水改造"]
[63,"活接头","DN32","镀锌","个",1,{"$nulls":3},"空压机冷却水改造"]
[64,"手动球阀","DN32 不锈钢",null,"个",1,{"$nulls":3},"空压机冷却水改造"]
[65,"润滑油","卓力\\HM46抗磨液压油",null,"桶",1,null,null,"长城"]
[66,"油漆（免除锈底漆）","水性免除锈底漆    桶/5KG",null,"桶",1]
[67,"油漆","耐高温金属漆（孔雀蓝）",null,"公斤",1,{"$nulls":3},"供热管道保温外壳美化"]
[68,"油漆","耐高温金属漆（草绿）",null,"公斤",1,{"$nulls":3},"供热管道保温外壳美化"]
[69,"油漆","耐高温金属漆（黑）300℃",null,"公斤",1,{"$nulls":3},"供热管道保温外壳美化"]
[70,"油漆","耐高温金属漆（黑）200℃  3KG/桶",null,"公斤",1]
[71,"油漆","黄色磁漆  3L/桶",null,"桶",1,{"$nulls":3},"检修耗材"]
[72,null,"大红磁漆  5L/桶",null,"桶",1]
[73,null,"天蓝色磁漆  3L/桶",null,"桶",1]
[74,null,"银色调和漆  2.5L/桶",null,"桶",1]
[75,null,"红丹防锈漆  4L/桶",null,"桶",1]
[76,"拇指滚刷","4寸 双黄（腈纶）配10支手柄  50支/袋",null,"袋",1]
[77,null,"8寸 双黄（腈纶）配10支手柄 30支/袋",null,"袋",1]
[78,"膨胀螺栓","φ10*80  50个/盒",null,"盒",1,{"$nulls":3},"现场检修用"]
[79,"螺母","304不锈钢 M4  1000只/盒",null,"盒",1]
[80,"螺栓（4.8级）","M8*45mm","碳钢","套",1,{"$nulls":3},"现场检修用"]
[81,null,"M10*35mm","碳钢","套",1,{"$nulls":3},"日常耗品"]
[82,null,"M12*40mm","碳钢","套",1]
[83,null,"M12*55mm","碳钢","套",1,{"$nulls":3},"日常耗品"]
[84,null,"M16*60mm","碳钢","套",1]
[85,null,"M16*120mm","碳钢","套",1]
[86,null,"M18*60mm","碳钢","套",1]
[87,null,"M18*70mm","碳钢","套",1]
[88,null,"M18*120mm","碳钢","套",1]
[89,"单头六角螺杆","M18*60mm 碳钢8.8级","碳钢8.8级","个",1,{"$nulls":3},"装载机用"]
[90,"钻尾自攻螺丝","铁镀锌M4.2*25",null,"只",1,{"$nulls":3},"耗品"]
[91,"钻尾自攻螺丝","铁镀锌M4.2*38",null,"只",1,{"$nulls":3},"耗品"]
[92,"不锈钢螺栓","M12*70mm(06cr25Ni20)","310S","套",1,{"$nulls":3},"锅炉挂砖专用"]
[93,"带帽螺栓","M8×80  8.8级",null,"套",1,{"$nulls":3},"日常维护检修"]
[94,"带帽螺栓","M10×80  8.8级",null,"套",1]
[95,"高压双头螺栓","M27×180  8.8级",null,"套",1,{"$nulls":3},"DN250流量计安装用"]
[96,"自攻燕尾钉","M4.2*25   100个/盒",null,"盒",1,{"$nulls":3},"现场检修用"]
[97,"自攻螺钉","M4.0*30   100个/盒",null,"盒",1]
[98,"迷你管卡钉","直径20mm，长27mm  火药头直径7.3mm 100个/盒",null,"盒",1]
[99,"迷你小圆片钉","火药头直径7.3mm 长度27mm 100个/盒",null,"盒",1]
[100,"膜片","减压阀配件（25公斤）",null,"片",1]
[101,"棉布袋（厚）","φ500mm*1100mm",null,"个",1,{"$nulls":3},"灰库放灰使用"]
[102,"开关电源","DR-120-24    输入：220VAC；\n输出：24VDC   5A",null,"个",1,null,null,"明纬"]
[103,"企业级8口千兆交换机","S1700-8G-AC",null,"个",1,null,null,"华为"]
[104,"斜口钳","5英寸",null,"把",1,null,null,"得力","旧换新"]
[105,"尖嘴钳","5英寸",null,"把",1]
[106,"老虎钳","4.5英寸~5英寸",null,"把",1]
[107,"压缩空气管","φ16*12  100米/箱",null,"箱",1,null,null,"亚德客","现场检修用"]
[108,null,"φ8*5   100米/箱",null,"箱",1,{"$nulls":3},"现场检修用"]
[109,"外牙快速接头直接","外径10转外牙4分",null,"个",1,{"$nulls":3},"现场检修用"]
[110,null,"外径12转外牙4分",null,"个",1,{"$nulls":3},"现场检修用"]
[111,"快速接头直接","φ12转φ10",null,"个",1,{"$nulls":3},"现场检修用"]
[112,null,"φ12转φ8",null,"个",1,{"$nulls":3},"现场检修用"]
[113,null,"φ16转φ12",null,"个",1,{"$nulls":3},"现场检修用"]
[114,"钢跳板","热镀锌 3000*25*45mm 厚度1.5mm",null,"个",1,{"$nulls":3},"脚手架"]
[115,"钢跳板","热镀锌 2000*25*45mm 厚度1.5mm",null,"个",1,{"$nulls":3},"脚手架"]
[116,"钢跳板","热镀锌 1500*25*45mm 厚度1.5mm",null,"个",1,{"$nulls":3},"脚手架"]
[117,"转速表","6236P+充电套装",null,"件",1,null,null,"胜利","测速用"]
[118,"中间继电器","JZ-7GJ-S220，AC220V",null,"只",1,null,null,"江阴新长江继电","化水控制箱"]
[119,"中间继电器","JZ-7GJ-S550，AC220V",null,"只",1,null,null,"江阴新长江继电","化水控制箱"]
[120,"陶瓷灯座","E27,7字，铜镀镍，全牙款",null,"只",1]
[121,"液压拉马顶针","M10；普通款+加长款51mm+超长款96mm各2支",null,"件",1]
[122,"撬棍","24英寸30度角 95-251-23长度600mm CR-V合金钢",null,"件",1,null,null,"史丹利"]
[123,null,"36英寸30度角 95-253-23长度900mm CR-V合金钢",null,"件",1,null,null,"史丹利"]
[124,"人字梯","2米 C型（100kg）",null,"件",1]
[125,"棘轮螺丝批组套","37件套05496A",null,"件",1,null,null,"世达"]
[126,"闭锁电磁铁","DC220V 华电VEP断路器",null,"件",1,null,null,"厦门华电开关有限公司"]
[127,"绝缘胶带","3M1600    黑色",null,"卷",1]
[128,"亚克力圆管","配套10个密封圈，外径19mm，长度1.2m",null,"根",1]
[129,"不锈钢压力表","Y-150   -0.1~0.15MPA",null,"个",1,null,null,"北京布莱迪","现场用"]
[130,"手持式水基型灭火器","1kg及以下 （需提供经销单位营业执照，该批次灭火器出厂合格证 、产品型式试验报告、消防认证标示、中国国家强制产品认证证书）","/","个",1,{"$nulls":3},"消防安全应急物资"]
[131,"氧化铝","3-5mm",null,"kg",1,{"$nulls":3},"干燥机"]
[132,"白色塑料取样桶  （带盖）","茶花牌（5公斤）",null,"个",1,{"$nulls":3},"化验使用"]
[133,"电动抽油泵      （充电式）","含24V锂电池、功率500W  配10米油管",null,"台",1,{"$nulls":3},"燃运使用"]
[134,"非接触式红外测温仪","UT300S  -32℃～340℃",null,"把",1,{"$nulls":3},"外管使用"]
[135,"液晶监视器    （VGA接口）","H321     32英寸",null,"台",1,null,null,"惠浦","厂区监控用"]
[136,"不锈钢压力表","Y-100   0~1.0MPA   1.0级  M20*1.5",null,"个",1,null,null,"布莱迪"]
[137,"充电式手电钻","GSB185-LI 2.0Ah一电一充",null,"套",1,null,null,"博世"]
[138,"行程开关","LX19-001",null,"只",1,null,null,"天正电气","灰渣设备"]
[139,"冲击钻头","圆柄6*110",null,"只",1]
[140,"铅酸蓄电池充电器","6897NV,12V/24V通用,40A",null,"只",1,null,null,"纽福克斯","升降机等铅酸蓄电池充电用"]
[141,"品字插座插口","一套公母对接：插座带盖,长1米，（安装孔距40mm配套3芯（纯铜）； 4平直插头，长35厘米",null,"套",1,{"$nulls":3},"升降机等铅酸蓄电池充电用"]
[142,"公牛电工绝缘胶布","18米/个",null,"个",1,null,null,"公牛","检修用"]
[143,"聚四氟乙烯生料带","DL389515      15m*12mm*0.1mm",null,"个",1,null,null,"得力"]
[144,"手持无极调温热风枪","型号：6511，2500W，数字显示温度",null,"支",1,null,null,"艾瑞泽"]
[145,"轴承","6204RZ",null,"套",1,null,null,"SKF"]
[146,"变径接头","1分外*2分内丝变径接头，黄铜材质",null,"只",1]
[147,"接触器","LC1 D95M7C",null,"只",1,null,null,"施耐德","抽屉柜"]
[148,"热继电器","LRD-3363C 63-80A",null,"只",1,null,null,"施耐德","抽屉柜"]
[149,"无线门禁套装","祖程X12套装6号，无线主机，门禁电源，磁力锁*2，ZL支架*2，ID卡*10，开关按钮",null,"套",1,null,null,"祖程","配电室"]
[150,"无线门禁套装","祖程X12套装10号，无线主机，门禁电源，磁力锁，L支架，ID卡*10，开关按钮",null,"套",1,null,null,"祖程","配电室"]
[151,"消防水带","8-65-25（含接头，不锈钢喉箍安装，有衬里聚氨酯）25米/条，检验报告，消防S码","涤纶长丝","条",1,{"$nulls":3},"消防器材更换"]
[152,"消防水带不锈钢喉箍","适用于8-65-25消防水带接头","不锈钢","个",1]
[153,"消防喷淋头","DN15,下喷洒水喷头，68℃动作",null,"个",1,{"$nulls":3},"输煤系统消防喷淋"]
[154,"分体式铁皮档案柜"," 860*400*380mm","铁","个",1,{"$nulls":3},"安全档案资料存放"]
[155,"应急物资柜1.2","厚度2mm   80*50*35 ","304不锈钢 ","个",1,{"$nulls":3},"现场应急物资柜"]
[156,"配电室挡鼠板，配卡槽及反光条（定制）","86*50cm   厚度25mm","铝合金","块",1]
[null,null,"296*50cm  厚度25mm",null,"块",1]
[null,null,"117*50cm  厚度25mm",null,"块",1]
[null,null,"114*50cm  厚度25mm",null,"块",1]
[null,null,"94*50cm   厚度25mm",null,"块",1]
[null,null,"116*50cm  厚度25mm",null,"块",1]
[null,null,"95*50cm   厚度25mm",null,"块",1]
[null,null,"115*50cm  厚度25mm",null,"块",1]
[null,null,"96*50cm   厚度25mm",null,"块",1]
[null,null,"118*50cm  厚度25mm",null,"块",1]
[null,null,"116*50cm  厚度25mm",null,"块",1]
[null,null,"146*50cm  厚度25mm",null,"块",1]
[null,null,"85.5*50cm  厚度25mm",null,"块",1]
[169,"挡板（定制）","145.5*60.5厚度25mm，高60.5cm，长度规格定制。","铝合金","块",1]
[null,null,"146.5*60.5厚度25mm，高60.5cm，长度规格定制。",null,"块",1]
[171,"中间继电器","JZ-7GJ-S220，AC220V",null,"只",1,null,null,"江阴新长江继电","化水控制箱"]
[172,"中间继电器","JZ-7GJ-S550，AC220V",null,"只",1,{"$nulls":3},"化水控制箱"]
[173,"编织袋","1100*1500mm",null,"个",1]
[174,"草皮","20*20CM",null,"提",1]
[175,"绿皮地毯","2m*15m",null,"平方",1]
[176,"草坪种子","500克/袋",null,"袋",1]
[177,"高清红外热成像仪","H21Pro[3.2吋 256*192双光融合",null,"台",1]
[178,"不锈钢板（定制）","厚1.5mm  宽度200mm 长度1900mm  ",304,"片",1,null,null,"定制","变压器边缘封堵"]
[179,null,"厚1.5mm  宽度170mm 长度1900mm  ",304,"片",1]
[180,null,"厚1.5mm  宽度150mm 长度1900mm  ",304,"片",1]
[181,null,"厚1.5mm  宽度170mm 长度1250mm  ",304,"片",1]
[182,null,"厚1.5mm  宽度170mm 长度250 mm ",304,"片",1]
[183,"直角型不锈钢板（定制）","厚1.5mm  角190mm*角44mm 长度1250 mm ",304,"片",1]
[184,null,"厚1.5mm  角190mm*角44mm 长度250 mm ",304,"片",1]
[185,null,"厚1.5mm  角150mm*角52mm 长度1250 mm ",304,"片",1]
[186,null,"厚1.5mm  角150mm*角52mm 长度250 mm ",304,"片",1]
[187,null,"厚1.5mm  角110mm*角52mm 长度1900 mm ",304,"片",1]
[188,null,"厚1.5mm  角110mm*角110mm 长度1250 mm ",304,"片",1]
[189,"配电室挡鼠板","铝合金，长86*高50cm,厚度25mm，配卡槽及反光条",null,"块",1]
[190,null,"铝合金，长116.5*高50cm,厚度25mm，配卡槽及反光条",null,"块",1]
[191,"轴承","6313C3   无挡环",null,"套",1,null,null,"SKF","备件"]
[192,"双网金属切割片","ø105*1.2*16mm",null,"盒",1,null,null,"银象","日常耗品"]
[193,"试验型接线端子","SKJ-6S",null,"只",1,null,null,"SMS施米斯","耗品"]
[194,"连接件","SFB1 10-RTK/S",null,"只",1]
[195,"终端固定件","SKJ-2G2",null,"只",1]
[196,"终端隔板","SKJ-6SG",null,"只",1]
[197,"监控屏幕","32寸   壁挂   BNC接口视频信号输入",null,"台",1,{"$nulls":3},"汽包水位屏幕更换"]
[198,"模拟视频画面分割器","4进二出    BNC接口",null,"个",1]
[199,"指示灯","XB2-BVQ3LC 380V 绿色",null,"只",1,null,null,"施耐德","耗品"]
[200,null,"XB2-BVQ4LC  380V 红色",null,"只",1,null,null,"施耐德"]
[201,null,"XB2-BVQ5LC   380V 黄色",null,"只",1,null,null,"施耐德"]
[202,"电力电缆","YJV22-3*10+2*6",null,"米",1,null,null,"上海远东、太阳电缆","雨水井水泵"]
[203,"企业级\n8口千兆交换机","S1700-8G-AC",null,"个",1,null,null,"华为","厂内办公、生产、监控网络维护用"]
[204,"无线路由器","TP-LINK-AX5400",null,"台",1,null,null,"TP-LINK"]
[205,"高精密电阻","250R   250Ω",null,"个",1,null,null,"厦门宇电自动化科技有限公司","维修、信号转换用"]
[206,"气缸","长375mm，边长138mm，工作行程：300mm  0.4Mpa~0.6Mpa;配Y型接头",null,"个",1,{"$nulls":3},"现场维修用"]
[207,"梅花敲击扳手","30mm",null,"把",1,{"$nulls":3},"公用工具"]
[208,null,"32mm",null,"把",1]
[209,"开口敲击扳手","30mm",null,"把",1]
[210,null,"32mm",null,"把",1]
[211,"20V无刷往复锯","DCJF22强力6.0（配木材刀1片，金属锯条2片）",null,"把",1,null,null,"东成"]
[212,"电焊钳","A250",null,"把",1,null,null,"东成"]
[213,"高频氩弧焊把","QQ-300气电分离（16平方6米）",null,"把",1,null,null,"安德利","公用工具"]
[214,null,"QQ-150气电分离（6平方6米）",null,"把",1,null,null,"安德利"]
[215,"不锈钢气动梭阀","CF8   DN25  PN16",null,"个",1,{"$nulls":3},"输灰用"]
[216,null,"CF8   DN32  PN16",null,"个",1]
[217,"不锈钢焊条","（A402) E310-16  2.5mm",null,"箱",1,null,null,"金桥","日常耗品"]
[218,null," (A402) E310-16  3.2mm",null,"箱",1,null,null,"金桥"]
[219,null," (A102) E308-16  2.5mm",null,"箱",1,null,null,"金桥"]
[220,null," (A102) E308-16  3.2mm",null,"箱",1,null,null,"金桥"]
[221,null,"(A302) E309-16  3.2mm",null,"箱",1,null,null,"金桥"]
[222,null,"(A302) E309-16  2.5mm",null,"箱",1,null,null,"金桥"]
[223,"碳钢焊条","J422  3.2mm",null,"箱",1,null,null,"金桥"]
[224,null,"J422  2.5mm",null,"箱",1,null,null,"金桥"]
[225,"金属缠绕垫片","DN25  PN25",null,"片",1]
[226,"八角缓冲垫","MT8","橡胶","个",1,{"$nulls":3},"燃运行车"]
[227,null,"MT4","橡胶","个",1,{"$nulls":3},"水泵用"]
[228,"机械密封","108U-60","W-W","个",1,{"$nulls":3},"清水泵用"]
[229,"地漏过滤网","适用110PVC管",304,"个",1,{"$nulls":3},"各条皮带排水口用"]
[230,"排水沟铁篦子（沟盖板）","750mm*450mm*50mm","球墨铸铁篦子","块",1,null,null,"沧州弋嘉","厂区道路排水坑盖板"]
[231,null,"600mm*400mm*50mm",null,"块",1,{"$nulls":3},"进灰库沟盖板"]
[232,"吊装带","3吨，3米",null,"条",1,{"$nulls":3},"日常耗品"]
[233,null,"3吨，2米",null,"条",1]
[234,"高空安全带","双背双绳小钩  3米",null,"条",1]
[235,null,"双背双绳小钩  2米",null,"条",1]
[236,"塑料膨胀管   （塑料米）","M6    100个/盒",null,"盒",1]
[237,"尼龙扎带","5.0*200    200根/包",null,"包",1,{"$nulls":3},"现场维修用"]
[238,null,"5.0*400    200根/包",null,"包",1,{"$nulls":3},"现场维修用"]
[239,"松动除锈剂","大瓶   450ml",null,"瓶",1,{"$nulls":3},"日常耗品"]
[240,"S型绝缘电缆挂钩","中号（承重8公斤）",null,"个",1,{"$nulls":3},"厂区电缆沟使用"]
[241,"取样铲","长柄300*300*130mm",null,"把",1,{"$nulls":3},"燃运使用"]
[242,"安全帽","黄色 印字（环保能源）",null,"个",1,null,null,"霍尼韦尔","运行部使用"]
[243,"纠偏机挡轮","JBL-B","铁","个",1,null,null,"南通天诚电力设备有限公司","燃运皮带用"]
[244,"可塑料","配套复合剂 （另增加4桶复合剂 ）",null,"吨",1,{"$nulls":3},"锅炉耗材"]
[245,"打滑检测仪表","BX-SA  含一次检测元件与二次显示控制仪  安装模式及样品看现场",null,"套",1,null,null,"徐州标鑫测控设备、施迈赛，松岛","燃运皮带打滑检修用"]
[246,"过渡管","108*6mm/168*16mm                 （图号57CS34-1-0）","20G","个",1,null,null,"华西能源","锅炉省煤器进口管段"]
[247,"《防止电力生产事故的二十五项重点要求及编制释义》","2023版","平转","本",1,{"$nulls":3},"安全学习培训材料"]
[248,"色带 ","兄弟 12mm 黄底",null,"个",1,null,null,"兄弟","日常耗材"]
[249,"色带 ","兄弟 24mm 黄底",null,"个",1,null,null,"兄弟","日常耗材"]
[250,"色带 ","兄弟 36mm 黄底",null,"个",1,null,null,"兄弟","日常耗材"]
[251,"激光笔","得力 DL552004",null,"个",1,null,null,"得力","锅炉检修"]
[252,"邑固正压式消防空气呼吸器备用瓶","6.8L碳纤维防爆高压气瓶带阀带气（气瓶出厂检验日期需为2023年）","碳纤维","个",1,{"$nulls":3},"应急物资"]
[253,"锄头","10.5cm*23cm(30cm含柄高)\n重约1.9斤含木柄","轨道钢","把",1]
[254,"锄头","15cm*19cm(27cm含柄高)\n重约2.4斤含木柄\n","轨道钢","把",1]
[255,"小尖铲","19cm*32.5cm(42.5cm含柄高)含木柄\n","锰钢","把",1]
[256,"尖铲","23cm*30cm(42.5cm含柄高)\n含木柄\n","锰钢","把",1]
[257,"水泵叶轮螺母（含垫片、弹簧垫）","M27*1.5（牙距）","不锈钢CF3M","个",1,{"$nulls":3},"化水水泵用"]
[258,"硅橡胶板","4mm（厚）","硅橡胶","平方",1,{"$nulls":3},"检修耗材"]
[259,"全不锈钢挂锁","户外不锈钢挂锁；防锈；高：50mm；短梁；一把钥匙统开",null,"把",1,{"$nulls":3},"外管仪表箱锁头更换"]
[260,"六角缓冲垫","T154",null,"个",1,{"$nulls":3},"化水水泵用"]
[261,"防滑垫","长13M*宽0.9M*厚2.5MM",null,"块",1,{"$nulls":3},"水处理使用"]
[262,"钢丝轮","内孔16mm  (适用100型角磨机）",null,"个",1,{"$nulls":3},"日常耗材"]
[263,"百叶片","(适用100型角磨机）",null,"片",1,{"$nulls":3},"日常耗材"]
[264,"骨架油封","80*105*12",null,"个",1,{"$nulls":3},"冷渣机减速箱用"]
[265,"低压试电笔","C-MART L0036",null,"支",1]
[266,"警示带","正在施工 注意安全 50米",null,"卷",1,{"$nulls":3},"锅炉检修"]
[267,"手电","SZSW2105",null,"个",1,null,null,"尚为","锅炉检修"]
[268,"微型防爆头灯","RTD8116，DC3.7V 3W,容量4.4Ah；放电时间：强光大于8小时、工作光大于16小时；IP66；帽配方式，",null,"只",1,null,null,"日昇之光","检修工作用"]
[269,"检修工作行灯","橡皮行灯，铁丝带挂勾，E27陶瓷灯头铜镀镍全牙款，不带开关、不带电源线、橡胶柄。",null,"只",1,{"$nulls":3},"检修工作照明用"]
[270,"LED球泡灯","12W 12VAC/DC  E27",null,"只",1,{"$nulls":3},"检修工作照明用"]
[271,"端子透明盖板","TC60A/4P",null,"只",1,{"$nulls":3},"易损件"]
[272,"端子","TC60A/4P",null,"只",1,{"$nulls":3},"检修箱用"]
[273,"导轨式接线端子","IN30BK",null,"只",1,{"$nulls":3},"检修箱用"]
[274,"LED面板灯","YDP60*60C1-LED36   6500K",null,"只",1,null,null,"FSL佛山照明","办公楼及厂房"]
[275,"电线连接头","万特弗LT211 ,250V 32A 橙色透明一进一出",null,"只",1,{"$nulls":3},"耗品"]
[276,"彩色摄像机","DS-2CE16D1T  3.6mm   模拟信号输出",null,"个",1,null,null,"海康威视","现场维修、增加"]
[277,"彩色摄像机","DS-2CE16D1T   6mm    模拟信号输出",null,"个",1]
[278,"警示牌","正在施工 注意安全",null,"块",1,{"$nulls":3},"锅炉检修"]
[279,"五点式安全带 ","GM3663 静态负荷大于15KN绳长1.8m（LA标志）  ",null,"条",1,{"$nulls":3},"日常检修"]
[280,"重型工具柜","通体四层无挂板H1800*W1000*D500mm，可调节隔板，单层承重150KG,灰白色，冷轧钢板1.2mm厚（门不带孔）",null,"只",1,{"$nulls":3},"配电室存物柜"]
[281,"安全工器具柜","H1500*W800*D450,灰白色，\n冷轧钢板1.0mm厚",null,"只",1,{"$nulls":3},"水工、公用配电室"]
[282,"压力表","Y-40Z   轴向安装   0~1.0MPA  ",null,"个",1,null,null,"北京布莱迪仪器仪表","气动元件用"]
[283,"不锈钢压力表","Y-100，0~1.0MPA，1.0级；M20*1.5，含市所检定证书",null,"个",1,{"$nulls":3},"强检压力表更换"]
[284,"锅炉汽包不锈钢压力表","Y-150  0~10mpa，过程接口M20*1.5，径向安装，材质316L，精度1.0级，安全玻璃（含市所检定证书）",null,"个",1]
[285,"锅炉汽包不锈钢压力表","Y-150  0~10mpa，过程接口M20*1.5，径向安装，材质316L，精度1.0级，安全玻璃（含市所检定证书）刻度盘上画红色线：高值：4.31MPA；低值：3.82MPA",null,"个",1]
[286,"锅炉集汽集箱不锈钢压力表","Y-150  0~6mpa，过程接口M20*1.5，径向安装，材质316L，精度1.0级，安全玻璃（含市所检定证书）刻度盘上画红色线：高值：3.92MPA；低值：3.43MPA\n",null,"个",1]
[287,"绝缘手套","10KV绝缘手套(含具备承试资质的第三方检测报告）",null,"双",1,{"$nulls":3},"水工、公用配电室"]
[288,"绝缘靴","10KV绝缘靴43码(含具备承试资质的第三方检测报告）",null,"双",1,{"$nulls":3},"水工、公用配电室"]
[289,"高压验电笔","GSY-10国标(含具备承试资质的第三方检测报告）",null,"只",1,{"$nulls":3},"水工、公用配电室"]
[290,"便携式超声波测厚仪","GE便携式超声波测厚仪DM5E DL数显基本型  配DA512型探头",null,"台",1,null,null,"GE","金属测厚"]
[291,"臭氧浓度仪","在线测量，紫外灯管原理，量程;0~300mg/L  输出：4~20MADC  电源220VAC  ",null,"台",1,null,null,"青岛朗科  新大陆  IDEAL","2#臭氧发生器用"]
[292,"脉冲除尘器布袋  （定制）","φ128（花板孔洞）*2100MM\n烧毛、防水、防油粉尘浓度出口≤60mg/nm³","氟美斯","条",1,{"$nulls":3},"石灰石中间仓布袋除尘器用"]
[293,"扁除尘布袋（定制）","异形风琴式扁布袋\nPE（ 550mg/㎡）厚度1.8mm+防油拒水后处理。长900mm*宽890mm*滤袋数量34个\n出风口外形尺寸（含压边）：1630mm*1100mm\n出口浓度<30mg/米³。\n内配304不锈钢弹簧，尺寸要求与滤袋匹配，不能与滤袋产生摩擦，重量要适重因本设备扁布袋为非标产品，尺寸需供应商现场再确认.","PE    550mg/㎡","套",1,null,null,"原江苏海峰电力机械集团股份有限公司","燃运输煤皮带粗碎细碎除尘器（JJPBC-36-A）配件"]
[294,"锅炉二次风水冷壁让管","图号57CS12-1-0（含监检报告）","20G GB/5310-2008","对",1,{"$nulls":3},"1#炉水冷壁二次风让管更换"]
[295,"试验型接线端子","SKJ-6S",null,"只",1,null,null,"SMS施米斯"]
[296,"限高牌（5米）","限高牌（5米）反光含配件",null,"个",1]
[297,"旧编织袋","500*700",null,"个",1,{"$nulls":3},"装床料及卫生清理"]
[298,"埋刮板机（配件）","Rms40头轮齿片",null,"个",1,null,null,"宜都双宜机电工程有限公司","刮板机头轮磨损更换"]
[299,"埋刮板机（配件）","Rms40尾轮",null,"个",1,{"$nulls":3},"刮板机尾轮磨损更换"]
[300,"在线式可燃气体检测仪","FGD2-C-EX  0-100%LEL  分辨率：0.1%LEL  24VDC  输出4~20MADC",null,"台",1,null,null,"深圳鑫海瑞","乙炔、柴油房易燃气体泄漏检测报警用"]
[301,"报警控制主机","CH100-C  接入信号4~20MADC  220VAC",null,"台",1]
[302,"踢脚板","3mm*120mm","A235","米",1]
[303,"传动轮（5槽B级）","外径18.5cm、内径4.7cm、宽10.5cm、每槽1.6cm.罗茨风机用",null,"个",1,{"$nulls":3},"风机"]
[304,"仿铜挂锁（不通开）","32mm",null,"个",1,{"$nulls":3},"运行部使用"]
[305,"仿铜挂锁（不通开）","50mm",null,"个",1,{"$nulls":3},"运行部使用"]
[306,"防尘半面罩","3M 3200黑胶升级版",null,"个",1,{"$nulls":3},"运行部劳保"]
[307,"全脸防护面罩","透明  型号：SG-81001",null,"副",1,{"$nulls":3},"应急物资"]
[308,"自吸过滤式防毒面具（全面罩)","3M 6800",null,"个",1,{"$nulls":3},"应急物资"]
[309,"滤毒盒","3M 6002CN",null,"对",1,{"$nulls":3},"应急物资"]
[310,"滤毒盒","3M 6004CN",null,"对",1,{"$nulls":3},"应急物资"]
[311,"自吸过滤式防毒面具（半面罩)","3M 6200 配：5N11CN滤棉 KN95级",null,"套",1,{"$nulls":3},"应急物资"]
[312,"电子秤（30KG）","ACS-19W  不锈钢秤盘+ABS仪表 \n分度值 0.1KG-1G（台秤）",null,"台",1,{"$nulls":3},"燃运使用"]
[313,"编织袋","800*500mm（旧）","尼龙","个",1,{"$nulls":3},"化水装树脂，炉渣"]
[314,"换热器芯片（含垫片）","E100B(B)-0.8/150",null,"m²",1,{"$nulls":3},"1#、3#臭氧发生器冷却水换热器片增加"]
[315,"换热器配套螺杆","M24*750",null,"只",1]
[316,"管道刷","不锈钢丝缠绕尼龙毛刷（毛刷尺寸φ12x120mm，加手柄以后总长度约200mm",null,"把",1,{"$nulls":3},"冷油器、空冷器\n管束清洗"]
[317,"水泥","GB/T3183-2O17M32.5  50KG/包","水泥","包",1,{"$nulls":3},"检修耗材"]
[318,"堵漏王水泥","850克/包","水泥","包",1,{"$nulls":3},"检修耗材"]
[319,"尼龙棒（加工件）","φ22mm*L:70mm","尼龙","个",1,{"$nulls":3},"2#输煤皮带机用"]
[320,"尼龙棒（加工件）","φ24mm*L:70mm","尼龙","个",1,{"$nulls":3},"3#5#输煤皮带机用"]
[321,"室内消火栓","SN65(DN65)","锻钢","个",1,{"$nulls":3},"厂内消防用"]
[322,"钢丝绳卡","18mm","锻钢","个",1,{"$nulls":3},"干煤棚行车用"]
[323,"竹梯","6.5米","竹","把",1,{"$nulls":3},"细碎楼用"]
[324,"焊把电缆","16mm²","铜","米",1,{"$nulls":3},"焊机焊把线"]
[325,"警示带","正在施工注意安全50米/盘","尼龙","盘",1,{"$nulls":3},"检修用"]
[326,"排插","GN-311 4位分控全长3米， 超功率过载保护",null,"件",1]
[327,"地插 ","GD1Z223 全铜五孔10A 120*120mm 安装孔距：60mm",null,"件",1,null,null,"公牛","办公楼地插"]
[328,"LED面板灯","LDP01036019 ， 36W 5700K,60cm*60cm",null,"只",1,null,null,"OPPLE","办公楼及厂房"]
[329,"LED面板灯","LDPO103604B857，ldp01036020、36W,5700K,30cm*120cm",null,"只",1,null,null,"OPPLE","一期主控"]
[330,"LED面板灯","LDP0107202B857，ldp01072006、72W,5700K,60cm*120cm",null,"只",1,null,null,"OPPLE","一期主控"]
[331,"LED控制装置","ELG-200-36A 3Y恒压恒流型\n 输入100~240VAV,输出36V",null,"只",1,null,null,"MEAN WELL","LED灯电源用"]
[332,"吊扇","FC140-BA 56寸/1.4米",null,"只",1,null,null,"美的","一期加药间"]
[333,"壁挂风扇","FWA40YA ",null,"只",1,null,null,"美的","二期加药间"]
[334,"壁挂风扇","FWA40YA ",null,"只",1,null,null,"美的","热工班组"]
[335,"指示灯","XB2-BVQ1LC 380V 白色",null,"只",1,null,null,"施耐德","耗品"]
[336,"强力焊接胶","ND1020  AB组份  50ml",null,"只",1,null,null,"纽盾","粘接修补"]
[337,"黄黑反光贴","3M工程级 10cm*45.7m",null,"件",1,{"$nulls":3},"耗品"]
[338,"黄黑反光贴","3M工程级 5cm*45.7m",null,"件",1,{"$nulls":3},"耗品"]
[339,"威图柜锁","MS821不锈钢，无杆配钥匙",null,"件",1,null,null,"海坦锁具","低压变频柜"]
[340,"五点式安全带","国标（带LA标志）双大勾",null,"件",1]
[341,"小型断路器","iC65N D16/4P",null,"只",1,null,null,"施耐德"]
[342,"小型断路器","iC65N D25/4P",null,"只",1,null,null,"施耐德"]
[343,"小型断路器","iC65N D40/4P",null,"只",1,null,null,"施耐德"]
[344,"插座转换器","GN-9333【一转三】 分控开关",null,"件",1,null,null,"公牛"]
[345,"激光手电筒","LB162 外观黑（蓝光）2电一充 ",null,"件",1,null,null,"雷佰"]
[346,"绝缘胶垫","10kv，15m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[347,null,"10kv，12m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[348,null,"10kv，10m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[349,null,"10kv，9m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[350,null,"10kv，7m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[351,null,"10kv，5m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[352,null,"10kv，4m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[353,null,"10kv，3.1m*1m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[354,null,"10kv，6m*0.8m*5mm，红色，表面防滑条纹（附第三方检验报告）",null,"张",1,{"$nulls":3},"配电室"]
[355,"电线连接头","万特弗LT211 ,250V 32A 橙色透明一进一出",null,"只",1,{"$nulls":3},"耗品"]
[356,"高压接地线","JDX-YDGB   10kV，3*1米+3米25mm2(含具备承试资质的第三方检测报告）",null,"件",1,null,null,"金锐电力","安全工器具"]
[357,"高压接地线","JDX-YDNL  10kV，3*1米+3米25mm2，0.5米杆平口螺旋式(含具备承试资质的第三方检测报告）",null,"件",1,null,null,"金锐电力","安全工器具"]
[358,"联轴器柱销缓冲垫","18*35*9mm（圆形）","橡胶","个",1,{"$nulls":3},"日常耗材"]
[359,"联轴器柱销缓冲垫","14*27*7mm（圆形）","橡胶","个",1,{"$nulls":3},"日常耗材"]
[360,"不锈钢卡箍","16-25mm",304,"个",1,{"$nulls":3},"日常耗材"]
[361,"不锈钢卡箍","18-32mm",304,"个",1,{"$nulls":3},"日常耗材"]
[362,"不锈钢卡箍","46-70mm",304,"个",1,{"$nulls":3},"日常耗材"]
[363,"不锈钢卡箍","65-95mm  （65~89、72~95）各10个",304,"个",1,{"$nulls":3},"日常耗材"]
[364,"电动扳手","（6.0Ah2电一充）488H2全套筒",null,"台",1,null,null,"东成","日常用公用工具"]
[365,"双网金属切割片","ø105*1.2*16mm",null,"盒",1,{"$nulls":3},"日常耗材"]
[366,"955中性硅硐结构胶","黑色",null,"条",1,{"$nulls":3},"日常耗材"]
[367,"结构胶专用枪","（十一轴承）15寸",null,"把",1,{"$nulls":3},"日常用公用工具"]
[368,"焊机快速接头","10--25",null,"套",1,{"$nulls":3},"日常耗材"]
[369,"焊机快速接头","35-50",null,"套",1,{"$nulls":3},"日常耗材"]
[370,"黄铜液位计阀","螺纹接口6分",null,"个",1,{"$nulls":3},"疏水箱水位计用"]
[371,"黄铜液位计阀","螺纹接口4分",null,"个",1]
[372,"壁挂式机械温湿度计","TH602F",null,"个",1,null,null,"美德时","现场控制室用"]
[373,"温湿度计","9017白色、机械式 室内壁挂式",null,"只",1,null,null,"得力","配电室"]
[374,"侧装式耐腐蚀型磁翻柱液位计","UHZ519C14-P20B1R1D-2.2m  法兰通径DN20，PN1.6MPA,带变送输出  32%烧碱，密度1.35，常温，常压，材质可以304SS衬PP",null,"套",1,null,null,"上海妙迪仪表有限公司","化水碱罐现场液位更换"]
[375,"导料槽侧板","C1带式输送机 导料槽后段型号:PD650C2-18   导料槽左右两侧算一套","Q235内衬16Mn耐磨材料","套",1,null,null,"南通天诚电力设备有限公司","燃运2#输煤皮带用"]
[376,"清扫器犁头","H型清扫器犁头650mm*650mm","铁及合金制品","片",1,null,null,"原江苏海峰电力机械集团股份有限公司","燃运输煤皮带用"]
[377,"清扫器犁头","P型清扫器犁头650mm*650mm","铁及合金制品","片",1,{"$nulls":3},"燃运输煤皮带用"]
[378,"窗口双向对讲机",null,null,"套",1,{"$nulls":3},"运行部使用"]
[379,"高清红外热成像仪","H21Pro[3.2吋 256*192双光融合",null,"台",1,null,null,"海康威视（威影）"]
[380,"手提式干粉灭火器","MFZ/ABC4（灭火器需提供企业法人营业执照副本 - 产品出厂合格证 - 产品型式检验报告、消防认证标示、中国国家强制产品认证证书）","/","个",1,{"$nulls":3},"消防器材补充、更换"]
[381,"《防止电力生产事故的二十五项重点要求》","2023版","平转","本",1,{"$nulls":3},"安全学习培训材料"]
[382,"沙胶手套",null,null,"双",1,{"$nulls":3},"劳保"]
[383,"绝缘手套","12KV（含市所检定报告）",null,"双",1,{"$nulls":3},"劳保"]
[384,"消防灭火器检查卡记录卡卡套","宽10.5cm*高16cm，高透防水软膜  50套/捆","塑料","捆",1,{"$nulls":3},"安全物资"]
[385,"消防灭火器检查卡记录卡","宽9cm*高12cm，铜版纸   50张/套","纸质","套",1]
[386,"便携式热熔枪","热熔胶枪 GK-368带电池",null,"台",1]
[387,"热熔棒","10支/包",null,"包",1]
[388,"除草机","T23800两电一充（2580W功率）",null,"台",1,null,null,"雅马哈","运维工具"]
[389,"万用表","VC9820",null,"台",1,null,null,"胜利"]
[390,"禁止攀登警示牌","PVC（20*30cm)","PVC","块",1,{"$nulls":3},"安全物资"]
[391,"光伏板导水夹","30MM","铝","个",1,{"$nulls":3},"运维工具"]
[392,"钥匙密码盒","85*62*30mm",null,"个",1]
["电气工具配件类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"法兰静电跨接线","6平方BVR国标黄绿双色全长150mm孔径18mm   50根/包",null,"包",1,{"$nulls":3},"油泵房设备静电接地"]
[2,"法兰静电跨接线","6平方BVR国标黄绿双色全长150mm孔径12mm   50根/包",null,"包",1,{"$nulls":3},"油泵房设备静电接地"]
[3,"UPS触摸屏","SA-7A,DC24V(±15%),含XMI3140D-220V UPS（爱维达）监控软件",null,"只",1,{"$nulls":3},"4#UPS监控使用"]
[4,"低压电缆","YJV22-4*6",null,"米",1,null,null,"太阳牌","厂区路灯线路(综合楼至材料库段）短路更换"]
[5,"机械故障听诊器","KT7-117-122，主机/传感器/探头（锥形）/磁铁/耳机/便携包",null,"套",1,null,null,"克恩达（KENTA）","异响杂音检测维修工具"]
[6,"笔式测振仪","AR63C；配长、短探头各一根。",null,"个",1,null,null,"希玛"]
[7,"齿轮输油泵       （含配套电机）","2CY-2.1725 2.1m³/h 扬程250m 转速1480r/min",null,"台",1]
[8,"三相异步电动机","YE3-180M-4 18.5KW  380V IP55 IMB3 配SKF轴承 含注油孔",null,"台",1,null,null,"皖南","皮带输送机"]
[9,"电测表","PZ42-E3/KC 三相三线CT:2000A/5A,PT:AC100V,开关量8DI2DO+RS485通讯，辅助电源AC/DC85-270V",null,"只",1,null,null,"安科瑞","二期配电"]
[10,"变频器风扇","MMF-08D24ES  24VDC 0.16A D1915G1  RMB",null,"只",1,null,null,"MELCO二次风机富士变频器","二次风机富士变频器"]
[11,"散热风扇","UF-15PC23 BTH AC230V 50/60Hz，29W",null,"只",1,null,null,"FULLTECH"]
[12,"风机用三相异步电动机","YE3-132S2-2 7.5KW/380V,F级、IP55 SKF轴承，IMB3 轴伸端攻丝M10*30",null,"台",1,null,null,"六安/皖南/山东华力","燃运布袋除尘"]
[13,"铝壳变频三相异步电动机","YVP801-4  0.55kw,380v,IP55，IMB3",null,"台",1,null,null,"DELI得力电机","加药泵电机备用"]
[14,"变频器","ACS150-03E-03A3-4，PN：1.1KW、U1：3～380…480V、I1：6.0A、f1:48…63Hz、U2：3～0…U1V、I2：3.3A(150%1/10min）、f2:0…500Hz",null,"只",1,null,null,"ABB","化水加药泵"]
["热工仪表配件类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"智能型执行机构","2SB6012-2AD0-J02   \n推力：6400N   220VAC   4~20madc \n 配套安装支架",null,"台",1,null,null,"搜派师\n自动化科技、西博思、南京科远","配套6#RPT、\n10#RPT减温调节阀"]
[2,"焊接式减温调节阀","PN100，DN32mm，介质：热水，工作压力=5.8MPa，T=103度，Qmax=4t/h，常用流量：0.8~2t/h，最小流量：0t/h，力矩：1600~4000N，RPT进口蒸汽压力3.5MPA，蒸汽进口温度：450度，出口蒸汽压力：1.5~1.6MPA，温度：220~225度",null,"个",1,null,null,"江苏横河、鞍山工装、重庆川仪","6#RPT减温阀更换"]
[3,"焊接式减温调节阀","PN100，DN50mm，介质：热水，工作压力=5.8MPa，T=103度，Qmax=7t/h，常用流量：1.5~4t/h，最小流量：0t/h，力矩：1600~4000N，RPT进口蒸汽压力3.5MPA，蒸汽进口温度：450度，出口蒸汽压力：1.5~2.0MPA，温度：222~225度",null,"个",1,null,null,"江苏横河、鞍山工装、重庆川仪","10#RPT减温阀更换"]
[4,"MAC V5.2.5版SM202主控卡件","SM202主控卡件，MAC V5.2.5版（含DP主站软件1.0）",null,"个",1,null,null,"杭州和利时自动化有限公司","1#2#炉外脱硫除尘DCS系统主控卡件故障更换"]
[5,"数字智能调节器","  AI-708-I4-X3  面板：宽*高（80*160mm）；输入信号：4~20mADC；输出信号：4~20mADC；电源：220VAC  带PID调节功能；可实现自整定功能",null,"台",1,null,null,"厦门宇电自动化"]
[6,"针型阀","J21H-160P DN20   PN16.0MPa \n T:500度  石墨填料  外螺纹看样品",null,"个",1,null,null,"天长科迪","现场部分取压阀更换"]
[7,"焊接式仪表针型阀","J21H-160P   DN10   PN16.0MPa \n T:500度  石墨填料",null,"个",1]
[8,"外螺纹转接头","不锈钢，耐压：16MPA，耐温：500度，\n一端外螺纹：1/2NPT；一端为M20*1.5",null,"个",1,null,null,"天长科迪"]
[9,"高能点火器","JGD-20",null,"台",1,null,null,"江阴创捷电气设备有限公司","3#锅炉左侧点火装置更换"]
[10,"高压点火电缆","JDL-5000",null,"条",1]
[11,"高能点火枪","LDQ-L1200",null,"支",1]
[12,"压力变送器","   DMP305X-TST-S305GSSF 连接方式：M20*1.5，带HART、现场显示及设置按钮，0~2.5MPA，配不锈钢堵头",null,"台",1,null,null,"上海立格仪表自动化有限公司","现场检修用"]
[13,"硬盘录像机","DS-7916HQH-K4 16通道模拟信号输入、带1个视频模拟信号总输出口  每台各配硬盘： 4T",null,"台",1,null,null,"海康","127、124、128监控录像机故障更换"]
[14,"数字智能调节器","AI-708B  横式面板：高*宽（80*160mm）；  输入信号：4~20mADC；输出信号：4~20mADC；电源：220VAC  带PID调节功能；可实现自整定功能",null,"个",1,null,null,"厦门宇电自动化科技有限公司","现场数显仪表用"]
[15,"双金属温度计","径向安装，-40~80度，外螺纹M27*2  L=80mm",null,"个",1,null,null,"科迪"]
[16,"标准气体","SO2    2000mg/m3   8L",null,"瓶",1,null,null,"中国计量科学研究院","作为校验分\n析仪器用"]
[17,null,"SO2    1000mg/m3   8L",null,"瓶",1]
[18,null,"NO   800mg/m3   8L",null,"瓶",1]
[19,null,"O2  12.5%  8L",null,"瓶",1]
[20,null,"N2  99.999%  8L",null,"瓶",1]
[21,"多回转执行机构","2SA8821-5CE1  电源380VAC",null,"台",1,null,null,"搜派师自动化科技有限公司、西博思、西贝、PQL深圳万讯","1#炉外脱硫岛风门挡板"]
[22,"智能流量积算仪","MY-NHR-8602R-A-X-A-A-A-2P 电源：24VDC；带配电24VDC；带与我司传输系统软件通讯协议一样的485通讯  自动识别饱和与过热蒸汽计量",null,"台",1,null,null,"虹润","流量智能积算仪维护检修、送检更换用"]
[23,"压力调节阀(WY945H-100IDN100)","1、进口蒸汽：P：3.5MPa，T：435度  \n2、出口蒸汽：P：1.55~1.6MPa，T：222~225度 \n3、出口蒸汽最大流量：25t/h，出口蒸汽常用流量：8~12t/h，最小流量：0~3t/h，全关流量：0t/h\n4、调压阀：DN100  PN100\n5、流量特性:线性   行程:30mm  最大力矩：6400N\n6、根据工艺参数制造加工，如有不清楚可来电咨询\n配套现场RPT装置一体式直行程压力调节阀；带散热架，DN100，PN100；介质：蒸汽； 利用现场旧的鞍山工装执行机构进行调节，安装螺纹、孔洞要按照现场执行机构尺寸加工。","ZGZOCrMo","台",1,null,null,"杭州华惠","6#7#RPT配套厂家，调压阀检修更换"]
[24,"水泵户外控制箱","304不锈钢材质，宽度450mm*高度500mm*深度250mm，厚度1.5mm，按图配置制作",304,"只",1,{"$nulls":3},"雨水井水泵"]
[25,"雷达连续料位计","FMR57-AAACCABDA6YYY9+AK   带HART，两线制，喇叭100mm，显示操作：SD02 按键",null,"台",1,null,null,"E+H，VEGAPULS，FOXBORO","3#炉石灰仓料位检修用"]
[26,"磁浮式液位计","UTZ6.4F-TGXY    法兰连接，中心距：600mm    工作压力3.8MPA，工作温度：300度，连接法兰盘：PN100  DN25",null,"套",1,null,null,"铁岭铁光仪器仪表有限责任公司，\n德国AI，SOLIDAT","3#炉左侧双色水位计用"]
[27,"双室平衡容器"," TG-10-BSP  T：450度，PN100,DN20,L=600mm  取压在侧边",null,"个",1,null,null,"长春锅炉仪表程控设备股份有限公司","1#2#锅炉汽包水位用"]
[28,"压力变送器","\nDMP305X-TST-S305GSSF 连接方式：M20*1.5，带HART、现场显示及设置按钮，0~2.5MPA，配不锈钢堵头",null,"台",1,null,null,"上海立格仪表自动化有限公司  FOXBORO  罗斯蒙特","生产现场用"]
[29,"智能型执行机构","2SB6012-2AD0-J02   推力：6400N   220VAC   4~20madc  配套安装支架",null,"台",1,null,null,"搜派师自动化科技","配套7#RPT减温调节阀"]
[30,"焊接式减温调节阀","PN100，DN32mm，介质：热水，工作压力=5.8MPa，T=103度，Qmax=2.9t/h，常用流量：0.8~2t/h，最小流量：0t/h，力矩：1600~4000N，RPT进口蒸汽压力3.5MPA，蒸汽进口温度：450度，出口蒸汽压力：1.5~1.6MPA，温度：220~225度",null,"个",1,null,null,"江苏横河集团","7#RPT减温阀更换"]
[31,"智能压力变送器","DMP305X-TST-S305GSSF 连接方式：M20*1.5，带HART、现场显示及设置按钮，0~2.5MPA，配不锈钢堵头",null,"台",1,null,null,"上海立格仪表有限公司 FOXBORO  罗斯蒙特","厂内厂外日常送检更换用"]
[32,"铠装热电偶","WRNK-331 L=3000mm ；铠装偶外径ф8.0mm，材质为GH3039  K分度  ;0~1200℃;  配专用耐磨保护管长L=600mm，整根耐磨段材质为钨12%，钴28%、镍16%、铬18%、锰3%、硅1.5%等和其他微量元素一体铸成；外径:φ30,开孔:φ12（法兰盘：外径：160mm；开孔：φ18mm；孔距：130mm）;接线盒进线开口螺纹:M20*1.5;缆径:φ10",null,"支",1,null,null,"天长科迪，FOXBORO、重庆川仪","炉床温度检修"]
[33,"不锈钢转接头","外螺纹1/2NPT转外螺纹M20*1.5",null,"个",1,{"$nulls":3},"现场检修用"]
[34,"不锈钢双金属温度计","L=100mm，0~100度，M27*2",null,"支",1,{"$nulls":3},"2#汽机冷油器用"]
["专业配套设备配件类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"外伸缩防尘罩","1.材质:衬胶帆布+Q235B；2.φ620×2300 配SQJ-100t/h",null,"套",1,null,null,"无锡申泉电力设备有限公司","灰库放灰使用"]
[2,"内伸缩防尘罩","1.材质:工业帆布；2.φ360×2300 配SQJ-100t/h",null,"件",1,{"$nulls":3},"灰库放灰使用"]
[3,"钢制伸缩筒","1.含钢丝绳；2.数量:7节.配SQJ-100t/h",null,"套",1,{"$nulls":3},"灰库放灰使用"]
[4,"散装头","材质:Q235B；配SQJ-100t/h",null,"件",1,{"$nulls":3},"灰库放灰使用"]
[5,"支撑板（图号：57CS254-4）","1cr18ni9ti 120*60*5mm","06Cr18NillTi","块",1,{"$nulls":3},"锅炉穿墙管"]
[6,"均流板（图号57CS254-5-1\\3#)","1cr18ni9ti   1451*160*5mm","06Cr18NillTi","块",1,{"$nulls":3},"锅炉穿墙管"]
["阀门、安全阀、流量计、水泵类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"安全阀","A48Y-40C\n公称通径：100/125mm；流道直径65mm；压力等级：1.6-2.0Mpa；使用介质：蒸汽；介质温度：≤300℃","组合件","台",1,null,null,"建议使用质量\n相对稳定的电力企业通用品牌产品（如：哈锅、德莱赛、莱斯（天津有工厂）、斯派莎克）","6#RPT配套安全阀（一用一备，每年轮换）"]
[2,"安全阀","A28W-16tdn32压力等级0.7-1.0Mpa整定压力0.8Mpa",null,"只",1,{"$nulls":3},"压缩空气储罐"]
[3,"安全阀","A48Y-40C-200\n公称通径：200/250mm；流道直径65mm；压力等级：1.3-1.6Mpa；整定压力1.57Mpa；使用介质：蒸汽；介质温度：≤350℃(配套进出口法兰）","组合件","台",1,null,null,"建议使用质量\n相对稳定的电力企业通用品牌产品（如：哈锅、德莱赛、莱斯（天津有工厂）、斯派莎克）","3#RPTa配套安全阀"]
[4,"手动涡轮蝶阀","二级涡轮 D341X-16Q DN600(304无销板）衬EPDM QT450阀体",null,"个",1,null,null,"达沃斯","厂区雨总口防泄漏措施"]
[5,"双瓣式止回阀","H76W 压力1.6mpa 通径150mm温度≤200℃","WCB","个",1,null,null,"原武汉耐特阀门有限公司","1#炉回料改造"]
[6,"截止阀","Z41H-16C    DN80 PN16","碳钢","个",1,{"$nulls":3},"化水压缩空气隔离阀"]
[7,"蝶阀（法兰式）","带涡轮 DN150 1.6mpa","WCB","个",1,{"$nulls":3},"1#炉回料改造"]
[8,"蝶阀","WD371X-R(316L)\n对夹式涡轮耐酸碱蝶阀\nDN150mm1.6Mpa","不锈钢316L","个",1,{"$nulls":3},"化水用"]
[9,"涡轮蝶阀","D342X-16C  DN250\n配套法兰、螺栓、垫片","铸钢","个",1,{"$nulls":3},"工业冷却水回水至循环水池应急排放"]
[10,"涡轮蝶阀","D342X-16C  DN150\n配套法兰、螺栓、垫片","铸钢","个",1,{"$nulls":3},"臭氧系统冷却水回水至循环水池应急排放"]
[11,"潜水泵","转速：3000r/min功率：1.5KW 内径50mm","不锈钢","台",1,{"$nulls":3},"燃运用"]
[12,"水泵      （配套原支座）","125-100-400\n扬程：50m流量：100m³/h转速：1470r/min 自冷却  耐腐蚀,电机中心高度200mm，不含电机\n（YE3-200L-4；30KW）","CF8M","台",1,null,null,"无锡市恒河化工防腐设备有限公司","化水中间水泵"]
[13,"无堵塞潜水排污泵","65WQ25-36 Q25m³/h H36m N7.5kw 2900r/min,IP68 380V 50HZ 铸铁材质，铸铁叶轮，碳钢泵轴，机械密封，出口DN65 PN6RF 配2.5寸软管接头 电缆18m","铸铁","台",1,null,null,"上海凯程     ","厂区雨总口防泄漏措施"]
[14,"潜水泵","WQD20-15-1.5","不锈钢","台",1,null,null,"臣源","化水燃运各一台"]
[15,"一体化孔板流量计","一体化孔板SRIII ；DN40，常用压力1.1~1.4MPa，温度：190~210度；流量量程：0.01~1T/h，配套差压变送器。",null,"台",1,null,null,"天津润泰、斯派莎克、FOXBORO","外管用户流量安装"]
["化学试剂、器皿及药品类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"玻璃称量瓶（带盖）","30×50",null,"个",1,{"$nulls":3},"化验室使用"]
[2,null,"40×25",null,"个",1,{"$nulls":3},"化验室使用"]
[3,null,"70×35",null,"个",1,{"$nulls":3},"化验室使用"]
[4,"丙三醇","500ml",null,"瓶",1,{"$nulls":3},"化验室使用"]
[5,"白凡士林","500g",null,"瓶",1,{"$nulls":3},"化验室使用"]
[6,"50ml酸式滴定管","50ml",null,"根",1,{"$nulls":3},"化验室使用"]
[7,"实验室滴水架","PP材料",null,"个",1,{"$nulls":3},"化验室使用"]
[8,"标煤","GBW11104",null,"瓶",1,{"$nulls":3},"化验室使用"]
[9,"标煤","GBW11101",null,"瓶",1,{"$nulls":3},"化验室使用"]
[10,"橡胶手套","耐酸碱，M码",null,"双",1,{"$nulls":3},"运行部使用"]
[11,"玻璃移液管","10ml",null,"根",1,{"$nulls":3},"化验使用"]
[12,null,"20ml",null,"根",1,{"$nulls":3},"化验使用"]
[13,"乙醚分析纯","500ml/瓶",null,"瓶",1,{"$nulls":3},"化验使用"]
[14,"pH广泛试纸",null,null,"盒",1,{"$nulls":3},"化验室使用"]
[15,"秒表","普通",null,"个",1,{"$nulls":3},"化验使用"]
[16,"白大褂","长袖（165-170）",null,"件",1,{"$nulls":3},"化验使用"]
[17,null,"短袖（160-165）",null,"件",1,{"$nulls":3},"化验使用"]
[18,"卡尔·费休试剂","150ml/瓶  4瓶/套",null,"套",1,null,null,"北京时代新维\n测控设备","化验使用"]
[19,"石油醚分析纯","500ml/瓶 沸点60-90",null,"瓶",1,{"$nulls":3},"化验室使用"]
[20,"PH广泛试纸",null,null,"盒",1,{"$nulls":3},"化验室使用"]
[21,"磷酸三钠","25kg/包  98%",null,"包",1,{"$nulls":3},"化验室使用"]
[22,"挥发分坩埚","MAGD1-002(不含盖）MAG6600\n工业分析仪",null,"个",1,null,null,"长沙开元","化验室使用"]
[23,null,"MAGD1-002(盖）MAG6600\n工业分析仪",null,"个",1,{"$nulls":3},"化验室使用"]
[24,"量热仪点火装置(5E-AC/PL自动量热仪)","长电极组件（HW-06-03)5E-AC/PL自动量热仪",null,"套",1,null,null,"长沙开元","化验室使用"]
[25,null,"中心电极组件（HW-06-02)5E-AC/PL自动量热仪",null,"套",1,{"$nulls":3},"化验室使用"]
[26,"透明玻璃细口瓶（磨口）","容量1000ml",null,"个",1,{"$nulls":3},"化验室使用"]
[27,"氨水（化学纯）","含量（NH3)％:25～28\n2500ml/瓶",null,"箱",1,{"$nulls":3},"化验室使用"]
[28,"PH广泛试纸",null,null,"盒",1,{"$nulls":3},"化验室使用"]
[29,"标煤","GBW11101",null,"瓶",1,{"$nulls":3},"化验室使用"]
[30,"量热仪氧弹O型密封圈","60×5.7（mm)\nGB/T1235-1976",null,"个",1,null,null,"长沙开元\n仪器型号：5E-AC/PL","化验室使用"]
["劳保类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"绝缘鞋（6KV)","38（1）、39（7）、40（5）、41（3）、42（3）、43（2）",null,"双",1,{"$nulls":3},"劳保"]
[2,"高温鞋","38（1）、39（8）、40（4）、41（3）、42（3）、43（2）",null,"双",1,{"$nulls":3},"劳保"]
[3,"雨鞋(中统）","36（2）、38（1）、39（7）、40（3）、41（3）、42（3）、43（2）",null,"双",1,{"$nulls":3},"劳保"]
[4,"护目镜","3M1711",null,"个",1,{"$nulls":3},"劳保"]
[5,"护目镜","护目镜 鼻托升级款 型号：SG-60002",null,"个",1]
[6,"防护眼镜","3M防冲击、防水雾、防飞溅",null,"个",1,{"$nulls":3},"劳保"]
[7,"沙胶手套",null,null,"双",1,{"$nulls":3},"劳保"]
[8,"帆布手套",null,null,"双",1,{"$nulls":3},"劳保"]
[9,"短皮手套",null,null,"双",1,{"$nulls":3},"劳保"]
[10,"长皮手套",null,null,"双",1,{"$nulls":3},"劳保"]
[11,"耐酸碱手套","长35CM 防水防油耐酸碱 黑色 加厚",null,"副",1]
[12,"口罩","3M 9005 50个/盒 耳戴",null,"盒",1,{"$nulls":3},"劳保"]
[13,"口罩","3M 9541 25个/盒  耳戴",null,"盒",1,{"$nulls":3},"劳保"]
[14,"棉布工作服","薄M（4）、厚M（4)、薄L（6）、厚L（6）、薄XL(3)、厚XL（3）、薄XXL(4)、厚XXL(4)、",null,"套",1,{"$nulls":3},"劳保"]
[15,"电焊工作服","M(3)、L（3）、",null,"套",1,{"$nulls":3},"劳保"]
[16,"袖套",null,null,"付",1,{"$nulls":3},"劳保"]
[17,"披肩",null,null,"条",1,{"$nulls":3},"劳保"]
[18,"雨衣","S(1)\\M(3)、L（7）、XL(4)、XXL(6)、S(1)",null,"套",1,null,null,"天堂","劳保"]
[]
["定制产品类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"固定资产标签卡（定制）","9*14cm  防水不干胶",null,"张",1]
[2,"固定资产标签卡\n（空白）","9*14cm  防水不干胶",null,"张",1]
[3,"配电箱安全标识牌","PVC防水贴（自带背胶），20*30CM厚度0.1mm（内容定制）",null,"张",1,{"$nulls":3},"安全整改用"]
[4,"有限空间安全告知牌","    宽40cm*高30cm，厚度0.1cm，每片4个角钻0.3cm直径安装孔","铝质","片",1,{"$nulls":3},"现场安全标识"]
[5,"名称编号标识牌   （定制）","PVC防水贴（自带背胶）厚度0.1mm，\n内容定制30*20cm","PVC","张",1,{"$nulls":3},"现场设备标识"]
[6,null,"PVC防水贴（自带背胶）厚度0.1mm，\n内容定制20*10cm","PVC","张",1]
[7,null,"PVC防水贴（自带背胶）厚度0.1mm，\n内容定制40*5cm","PVC","张",1]
[8,null,"PVC防水贴（自带背胶）厚度0.1mm，\n内容定制25*15cm","PVC","张",1]
[9,null,"PVC防水贴（自带背胶）厚度0.1mm，\n内容定制40*6cm","PVC","张",1]
[10,null,"PVC防水贴（自带背胶）厚度0.1mm，\n内容定制30*6cm","PVC","张",1]
[11,null,"PVC防水贴（自带背胶）厚度0.1mm，\n内容定制50*5cm","PVC","张",1]
[12,null,"PVC防水贴（自带背胶）厚度0.1mm，\n内容定制30*8cm","PVC","张",1]
[13,"标示牌","厂用段配电室管理制度\n（泡沫板，高80cm，宽60cm）",null,"个",1,{"$nulls":3},"运行部使用"]
[14,null,"直流电源室出入管理规定\n（泡沫板，高80cm，宽60cm)",null,"个",1,{"$nulls":3},"运行部使用"]
[15,"危险废物标签","200*200mm","防水不干胶","张",1,null,null,"定制","根据《危险废物识别标志设置技术规范》要求对危废识别标志进行更新"]
[16,"危废贮存设施标志","300*186mm","1.5mm304不锈钢","张",1,null,null,"定制"]
[17,"危废贮存设施标志","900*558mm","1.5mm304不锈钢","张",1,null,null,"定制"]
[18,"供热管道\n安全告知卡（户外张贴）","400mm x 300mm，黄底红字（高温蒸汽管道，请勿逗留！注意高温。24小时供热值班联系电话：0592-6807507）","背胶贴纸","张",1,{"$nulls":3},"供热管道\n安全警示"]
[19,"标识牌","空瓶/满瓶/使用中（双面） 各10块 配链子  直径10cm","亚克力板","个",1,{"$nulls":3},"锅炉检修"]
[20,"标识牌","240*180mm 3mm 铝板 上部两小孔用于悬挂（锅炉）",null,"个",1,null,null,"定制"]
[21,null,"240*180mm 3mm 铝板 上部两小孔用于悬挂（起重）",null,"个",1,null,null,"定制"]
[22,null,"240*180mm 3mm 铝板 上部两小孔用于悬挂（管道）",null,"个",1,null,null,"定制"]
["燃料、气体类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"柴油","0#",null,"吨",1,{"$nulls":3},"运行部锅炉点火备用"]
[2,"氧气","氧气 包装容积:40L，纯度%(V/V)>99.5%，氧气充装压力:15士0.5Mpa，瓶身规格:219X1500",null,"瓶",1,{"$nulls":3},"化验室、检修用"]
[3,"乙炔","包装容积:40L，纯度%(V/V)≥98%，乙炔充装量:3士\n0.5Kg，充瓶压力:2Mpa，\n瓶身规格:240X1000",null,"瓶",1,{"$nulls":3},"一期吹灰器、检修用"]
[4,"氩气","包装容积:40L，纯度%(V/V)≥99.99%，氩气充装压力:15±0.5Mpa，瓶身规格:\n219X1500",null,"瓶",1,{"$nulls":3},"检修用"]

{"sheet":"同集1-6月采购备品备件","index":2,"n_rows":289,"n_cols":10,"rows_kept":289,"merged":[[0,0,0,9],[1,0,1,9],[161,0,161,9],[190,0,190,9],[202,0,202,9],[210,0,210,9],[219,0,219,9],[237,0,237,9],[240,9,248,9],[249,9,252,9],[256,0,256,9],[264,0,264,9]]}
["2023年1月~6月备品备件采购"]
["五金配件、管材类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"自吸过滤式防毒面具套件（含帆布包）","P-K-3（原4号中罐）",null,"套",1,{"$nulls":3},"SNCR区域应急防护"]
[2,"自吸过滤式防毒面具套件（含帆布包）","P-E-3（原7号中罐）",null,"套",1,{"$nulls":3},"亚氯酸钠区域应急防护"]
[3,"自吸过滤式防毒面具套件（含帆布包）","P-A-3（原3号中罐）",null,"套",1,{"$nulls":3},"燃气炉区域应急防护"]
[4,"耐酸碱防护面罩（含滤盒）",null,null,"件",1,{"$nulls":3},"化水车间应急防护"]
[5,"耐酸碱防护服",null,null,"件",1,{"$nulls":3},"化水车间、SNCR区域应急防护"]
[6,"编织袋","25公斤",null,"个",1,{"$nulls":3},"煤运"]
[7,"空气过滤器（滤芯）","8829001-469","复合件","只",1,null,null,"寿力","4#空压机保养更换"]
[8,"空压机油","Sul l ube32油（桶20L）"," ","桶",1,null,null,"寿力","4#空压机保养更换"]
[9,"油气分离器（次级）","02250048-734 ","复合件","只",1,null,null,"寿力","4#空压机保养更换"]
[10,"油气分离器（初级）","250034-085   ","复合件","只",1,null,null,"寿力","4#空压机保养更换"]
[11,"油过滤器","250025-526",null,"只",1,null,null,"寿力","4#空压机保养更换"]
[12,"防尘过滤罐","8020防尘盒KP100",null,"个",1,{"$nulls":3},"空气预热器清灰"]
[13,"安全绳","外径不低于12mm，30米/条","钢丝内芯，双钩","条",1,{"$nulls":3},"高空作业"]
[14,"铁锈转化剂","灰色",null,"公斤",1]
[15,"双面胶","厚泡沫",null,"卷",1,{"$nulls":3},"标识牌张贴"]
[16,"双面胶","薄",null,"卷",1,{"$nulls":3},"标识牌张贴"]
[17,"工业级台式砂轮机","S1E-FF-200",null,"台",1,null,null,"东成","检修电动工器具坏换新"]
[18,"日式防护眼镜（强化款）",null,null,"个",1,{"$nulls":3},"班组个人防护用品"]
[19,"橡胶防尘口罩+40片活性炭过滤棉","3200型",null,"套",1,{"$nulls":3},"班组个人防护用品"]
[20,"五点式安全带",null,null,"条",1,{"$nulls":3},"三点式更换为五点式安全带"]
[21,"干粉灭火器","MFZ/ABC2",null,"个",1,{"$nulls":3},"装载机、公车灭火器更换"]
[22,"警戒线隔离带","红白，100米/个",null,"个",1,{"$nulls":3},"施工现场围挡使用"]
[23,"希捷硬盘","ST4000VX0003",null,"块",1,{"$nulls":3},"监控"]
[24,"挂锁","SANKE 240",null,"把",1,{"$nulls":3},"外管"]
[25,"无线路由器","TP-LINK AX5400",null,"台",1,{"$nulls":3},"办公室"]
[26,"内带加强钢丝塑料软管","内径75mm",null,"米",1,{"$nulls":3},"盐酸罐泄漏检修"]
[27,"不锈钢螺栓","M16*70 316",null,"套",1,{"$nulls":3},"盐酸罐泄漏检修"]
[28,"机械密封","SZ-35/MST4",null,"套",1,{"$nulls":3},"卸酸泵维修"]
[29,"卸酸泵叶轮","泵型号SZ50-32-125SF26",null,"个",1,{"$nulls":3},"卸酸泵维修"]
[30,"锂电除尘鼓风机20v两电一充","DCQF02-28",null,"套",1,null,null,"东成","检修电动工器具"]
[31,"红色油漆",null,null,"kg",1,{"$nulls":3},"消防箱及管道油漆"]
[32,"透明手动黄油枪","容量600CC、管径60mm、压力12000",null,"把",1,{"$nulls":3},"运行现场使用"]
[33,"管钳","36寸",null,"把",1,{"$nulls":3},"运行现场使用"]
[34,"铁锈转化剂","灰色",null,"KG",1,{"$nulls":3},"锅炉检修"]
[35,"铁锈转化剂","蓝色",null,"KG",1,{"$nulls":3},"锅炉检修"]
[36,"铁锈转化漆","绿色",null,"kg",1,{"$nulls":3},"锅炉检修"]
[37,"五金工具箱套装",null,null,"箱",1]
[38,"调温塑料焊枪",null,null,"台",1,{"$nulls":3},"坏更换"]
[39,"金属石墨缠绕垫","DN200 PN25",null,"片",1,{"$nulls":3},"供热管网疏水"]
[40,"单头全牙螺杆(8.8级）","10mm*50mm",null,"套",1,{"$nulls":3},"检修易耗品"]
[41,"单头全牙螺杆(8.8级）","16mm*65mm",null,"套",1,{"$nulls":3},"检修易耗品"]
[42,"超五类水晶头三叉纯铜镀金","100个/盒",null,"盒",1]
[43,"RJ45网络直通头防雷款",null,null,"个",1]
[44,"K2接线子双刀","100个/盒",null,"盒",1]
[45,"海康威视12V 2A室外防水监控电源",null,null,"个",1]
[46,"丁腈手套（掌浸）","7寸",null,"付",1]
[47,"复式外压平衡波纹补偿器","1.6SHWP(F)150X16/16J","执行标准GB/T12777-2008波纹管材质：SUS316，波纹厚度及层数：1.0*3 外层钢管材质：Q235-B，补偿量132mm，预拉伸：52mm，补偿器总长度：2200mm","台",1,{"$nulls":3},"中药厂线（同顺支线）美淳厂区内补偿器更换"]
[48,"二氧化碳灭火器","MT3",null,"个",1,{"$nulls":3},"配电室增设灭火器"]
[49,"气动闸板阀","Z674H-16C DN40 PN16",null,"台",1,{"$nulls":3},"1.2#炉仓泵平衡阀"]
[50,"油漆涂料刷滚筒","6寸",null,"把",1,{"$nulls":3},"油漆专用"]
[51,"油漆涂料刷滚筒","8寸",null,"把",1,{"$nulls":3},"油漆专用"]
[52,"油漆涂料刷滚筒芯","6寸",null,"个",1,{"$nulls":3},"油漆专用"]
[53,"油漆涂料刷滚筒芯","8寸",null,"个",1,{"$nulls":3},"油漆专用"]
[54,"耐高温无尘石棉绳（扭绳）","16mm",null,"kg",1,{"$nulls":3},"检修易耗品"]
[55,"耐高温无尘石棉绳（扭绳）","18mm",null,"kg",1,{"$nulls":3},"检修易耗品"]
[56,"铅酸蓄电池","BT-6M 1.3AC 6V 1.3Ah/20HR",null,"个",1,{"$nulls":3},"外管流量计无线发送器"]
[57,"监控4路画面分屏器","同轴模拟视频",null,"个",1]
[58,"海康威视监控交换机","8口千兆",null,"个",1]
[59,"高压不锈钢304SS针型阀DN15内螺纹","J13W-160P",null,"个",1]
[60,"高压不锈钢304SS针型阀DN10","J23W-160P",null,"个",1]
[61,"双色水位计灯管长29.5cm","36v150w",null,"个",1]
[62,"下水道过滤网","75cm*45cm\n丝粗2mm，孔大1cm","不锈钢","块",1,{"$nulls":3},"厂区下水道井口过滤"]
[63,"海康威视摄像头","DS-2CE16C3T-IT3 6mm",null,"台",1,{"$nulls":3},"监控"]
[64,"世达电工老虎钳","6寸长152.4MM",null,"个",1]
[65,"塑料小桶5L","加厚PP(5L)",null,"个",1,{"$nulls":3},"取煤样"]
[66,"簸箕","加厚",null,"个",1,{"$nulls":3},"煤运"]
[67,"斗车实心胎",null,null,"个",1,{"$nulls":3},"煤运"]
[68,"斗车（实心胎）",null,null,"辆",1,{"$nulls":3},"煤运"]
[69,"热电偶","5E-MAG6700工业分析仪挥发份",null,"件",1,null,null,"长沙开元","备件"]
[70,"温湿度计","9013s  室内 挂式",null,"个",1,null,null,"得力","MCC配电室增加"]
[71,"放好封堵泥","1KG",null,"包",1,{"$nulls":3},"现场孔洞封堵"]
[72,"轴承","NSK 626Z",null,"个",1,null,null,"NSK","烟气监测真空泵"]
[73,"国标柔性有机防火泥","20公斤",null,"箱",1]
[74,"防火泥、密封胶泥白色",null,null,"包",1]
[75,"304不锈钢单头外丝管","DN65*100mm长",null,"根",1,{"$nulls":3},"干煤棚冲洗地板管腐蚀更换"]
[76,"电焊机焊把线快速接头","35—50型 红色.黑色插头",null,"套",1,{"$nulls":3},"检修工器具易耗品"]
[77,"射吸式割炬","G01-30  100型",null,"把",1,{"$nulls":3},"检修工器具易耗品"]
[78,"七彩跑马霓虹灯","LED ",null,"米",1,{"$nulls":3},"煤场更换"]
[79,"海康威视交换机8口千兆监控专用交换机","8口千兆",null,"个",1]
[80,"海康威视网络摄像头4MM200万","DS-2CD3T25D-I3",null,"个",1]
[81,"316不锈钢钢丝绳2毫米","2mm7*7结构",null,"米",1]
[82,"自动手摇喷漆","大红色",null,"瓶",1,{"$nulls":3},"外管网喷警示语"]
[83,"环形石墨填料","外径40mm*内径25mm*厚8mm",null,"个",1,{"$nulls":3},"仓泵出料阀阀芯密封件"]
[84,"三轮车充电器","60v20AH",null,"套",1,null,null,"超威","坏更换"]
[85,"金属石墨垫片","440mm*500mm*4.5mm",null,"片",1,{"$nulls":3},"仓泵钟罩阀"]
[86,"     干燥机冷媒","R407CKG",null,"瓶",1,{"$nulls":3},"5# 6#冷干机 "]
[87,"旁通阀","PTV12W",null,"支",1,{"$nulls":3},"6#冷干机 "]
[88,"热保护器","LE20MR",null,"只",1,{"$nulls":3},"6#冷干机"]
[89,"空压机油","Sul l ube32油（桶20L）",null,"桶",1,{"$nulls":3},"6#空压机补充油"]
[90,"高压石棉密封垫","1m宽*4m长*1mm厚",null,"米",1,{"$nulls":3},"检修易耗品"]
[91,"高压石棉密封垫","1m宽*4m长*3mm厚",null,"米",1,{"$nulls":3},"检修易耗品"]
[92,"DN200摆动阀陶瓷阀板",null,null,"个",1,{"$nulls":3},"原2#炉1#仓泵进料阀修复"]
[93,"DN200摆动阀连接杆含紧定螺丝及弹簧",null,null,"套",1,{"$nulls":3},"原2#炉1#仓泵进料阀修复"]
[94,"破布",null,null,"KG",1,{"$nulls":3},"检修易耗品"]
[95,"头灯","ok-5130A",null,"个",1,null,null,"海洋王","检修用"]
[96,"硅胶板","厚5mm",null,"㎡",1]
[97,"液氧罐爆破片","LFT30-1.76-50A   1.76Mpa",null,"个",1,null,null,"上海华理安全装备有限公司","到期更换"]
[98,"防水绝缘自粘带","J20 10KV",null,"卷",1,null,null,"3M","检修用"]
[99,"有尘石棉绳","20MM",null,"KG",1,{"$nulls":3},"锅炉检修"]
[100,"法兰连接橡胶软接头","DN200  PN16",null,"个",1,{"$nulls":3},"电除尘仓泵进口软接"]
[101,"304不锈钢螺杆","10mm*30mm长",null,"套",1,{"$nulls":3},"螺旋给煤机"]
[102,"304不锈钢螺杆","8mm*35mm长",null,"套",1,{"$nulls":3},"螺旋给煤机"]
[103,"油封","TC  85-110-12",null,"个",1,{"$nulls":3},"螺旋给煤机"]
[104,"耐油耐高温密封胶",null,null,"瓶",1,null,null,"卡夫特","检修易耗品"]
[105,"加厚耐磨百叶片","100mm",null,"片",1,{"$nulls":3},"检修易耗品"]
[106,"四方键销棒条"," 16mm*10mm","45＃钢   ","米",1,{"$nulls":3},"破碎机，筛网处理"]
[107,"环氧树脂","DY-E6011(A+B=2公斤/组)",null,"件",1]
[108,"PVC球阀","φ32",null,"个",1]
[109,"三插头","GNT-10S 10A 250V",null,"个",1,null,null,"公牛","检修用"]
[110,"防摔三插头","GNT-10S 10A 250V",null,"个",1,null,null,"公牛","检修用"]
[111,"五孔面板","250V 10A ",null,"个",1,null,null,"公牛","现场更换"]
[112,"五孔面板（带开关）","250V 10A ",null,"个",1,null,null,"公牛","现场更换"]
[113,"防火门闭门器","GA93-2CⅢ",null,"个",1,{"$nulls":3},"闭门器更新维护"]
[114,"角磨机不锈钢切割片","绿片107*1.2*16MM",null,"盒",1,{"$nulls":3},"检修易耗品"]
[115,"WD-40除锈剂400ML","24瓶",null,"箱",1,{"$nulls":3},"检修易耗品"]
[116,"海康威视网络摄像头6MM","200万像素室外枪式全彩",null,"个",1]
[117,"铝酸盐水泥","25Kg/袋","CA50   CA50-Ⅱ A600  ","袋",1,{"$nulls":3},"锅炉检修"]
[118,"管道箭头标识","10X2000CM","红底白箭头","卷",1,{"$nulls":3},"管道标识"]
[119,"管道箭头标识","10X2000CM","绿底白箭头","卷",1,{"$nulls":3},"管道标识"]
[120,"管道箭头标识","5X2000CM","红底白箭头","卷",1,{"$nulls":3},"管道标识"]
[121,"管道箭头标识","5X2000CM","绿底白箭头","卷",1,{"$nulls":3},"管道标识"]
[122,"管道箭头标识","5X2000CM","灰底黑箭头","卷",1,{"$nulls":3},"管道标识"]
[123,"管道流向标识","6x30CM","红底白字白箭头（蒸汽）","张",1,{"$nulls":3},"管道标识"]
[124,"管道流向标识","6x30CM","红底白字白箭头（疏水）","张",1,{"$nulls":3},"管道标识"]
[125,"管道流向标识","6x30CM","红底白字白箭头（排污）","张",1,{"$nulls":3},"管道标识"]
[126,"高温警示贴","15X20CM","黄底黑字 PP背胶","张",1,{"$nulls":3},"高温场所警示"]
[127,"防尘过滤罐",8020,null,"个",1,{"$nulls":3},"锅炉清灰用"]
[128,"高温警示板","400*500mm  铝板  ",null,"块",1,{"$nulls":3},"高温场所警示"]
[129,"环形裙边胶皮带","500*4（4+1.5）*7895",null,"条",1,{"$nulls":3},"3#计量给煤机老化更换"]
[130,"塑料浅盘","710×600×85(单位mm)",null,"个",1,{"$nulls":3},"主控、化水车间"]
[131,"加厚正方形塑料周转箱  加厚6#","570X570X250（单位 mm）",null,"个",1,{"$nulls":3},"燃气炉使用"]
[132,"防尘连体服","灰色、涤纶长丝+导电纤维",null,"套",1,{"$nulls":3},"生产运行"]
[133,"防静电高筒靴",null,null,"双",1,{"$nulls":3},"生产运行"]
[134,"不锈钢两轮斗车","117×67×47（单位cm )",null,"辆",1,{"$nulls":3},"燃运"]
[135,"遮阳伞","特大号",null,"把",1,{"$nulls":3},"燃运"]
[136,"风帽","按图制做","ZGCr25Ni20Si2W","个 ",1,{"$nulls":3},"锅炉检修"]
[137,"电控箱","380V 16A  自保持、热保护两路控制回路","304不锈钢 厚1.5mm","面",1,{"$nulls":3},"煤化验新增（安全提升）"]
[138,"玻璃胶","白色",null,"瓶",1,{"$nulls":3},"现场补缝用"]
[139,"强效免钉胶",null,null,"瓶",1,{"$nulls":3},"防鼠板安装"]
[140,"槽钢","8#  (80mm*43mm*5mm)","Q235B","米",1,{"$nulls":3},"电除尘锤头摆臂"]
[141,"U型加长抱箍（挡板）","12mm*内宽50mm*外高120mm","不锈钢","套",1,{"$nulls":3},"电除尘锤头摆臂"]
[142,"不烫手电焊钳","500A",null,"把",1,{"$nulls":3},"坏换新"]
[143,"金属石墨垫片内加强圈","125mm*90mm*5mm",null,"片",1,{"$nulls":3},"电动对空排阀盖"]
[144,"金属石墨缠绕垫","φ205*175*4.5mm",null,"个 ",1,{"$nulls":3},"锅炉检修"]
[145,"高压纯石墨盘根","10*10mm",null,"KG",1,{"$nulls":3},"锅炉检修"]
[146,"高压纯石墨盘根","6*6mm",null,"KG",1,{"$nulls":3},"锅炉检修"]
[147,"高压纯石墨盘根","4*4mm",null,"KG",1,{"$nulls":3},"锅炉检修"]
[148,"雨水排放口标识牌","30*50mm","铝板","个",1]
[149,"事故应急池标识牌","30*50mm","铝板","个",1]
[150,"中和池标识牌","30*50mm","铝板","个",1]
[151,"轴承","6208-2Z",null,"个",1,null,null,"SKF","炉外斜槽流化风机及备用"]
[152,"BOSS电动角磨机电机","RZ-8BAWA-AWG19.5X9",null,"个",1,{"$nulls":3},"坏换新"]
[153,"电除尘仓泵进料阀密封件","DN200","耐高温氟橡胶","个",1,{"$nulls":3},"坏换新"]
[154,"应急喷淋洗眼器",6610,"不锈钢","个",1]
[155,"炮钉枪","M900F ",null,"支",1,{"$nulls":3},"现场安装用"]
[156,"炮钉枪子弹","M900F ",null,"盒",1,{"$nulls":3},"现场安装用"]
[157]
[158]
["电气工具配件类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"控制盒","启动停止",null,"个",1,{"$nulls":3},"热机移动风机使用"]
[2,"配电箱面板","20位",null,"块",1,{"$nulls":3},"现场更换"]
[3,"应急指示灯","LED 220V 90min ",null,"个",1,{"$nulls":3},"安全整改"]
[4,"线槽","高10mm，宽20mm","PVC","米",1,{"$nulls":3},"现场新增线路用"]
[5,"静电夹","304 15米螺旋线",null,"条",1,{"$nulls":3},"易燃易爆卸车安全整改"]
[6,"绝缘垫","10KV 0.5mm*10m",null,"卷",1,{"$nulls":3},"安全整改"]
[7,"ABB端子组件","F121GCE710",null,"个",1,{"$nulls":3},"10KV开关更换"]
[8,"防爆型行程开关","BZX51-5L 5A 380V  IP54",null,"个",1,{"$nulls":3},"计量给煤机更换"]
[9,"LED平板灯","60*60cm 220v 36w",null,"个",1,{"$nulls":3},"煤化验更换"]
[10,"绝缘鞋","10KV",null,"双",1,{"$nulls":3},"安全整改"]
[11,"绝缘手套","10KV",null,"双",1,{"$nulls":3},"安全整改"]
[12,"电流试验端子","URTK/6S",null,"个",1,{"$nulls":3},"现场更换用"]
[13,"线路保护板","2.0mm 长*宽*高 3m*0.65m*0.4m ","热镀锌板","块",1,{"$nulls":3},"循变室竖井安全整改"]
[14,"漏电相位检测仪","10A/16A通用",null,"个",1,null,null,"德力西","全厂漏电检测用"]
[15,"尼龙开口软管","SPT-CPA6-PA23 φ25",null,"米",1,null,null,"上海蓝科","现场保护管更换"]
[16,"尼龙开口软管","SPT-CPA6-PA23 φ32",null,"米",1,null,null,"上海蓝科","现场保护管更换"]
[17,"防小动物板","1.8m*0.4m  黑黄条纹","铝合金","块",1,{"$nulls":3},"电除尘安全整改"]
[18,"防小动物板","0.83m*0.4m  黑黄条纹","铝合金","块",1,{"$nulls":3},"公用水安全整改"]
[19,"防小动物板","0.82m*0.4m  黑黄条纹","铝合金","块",1,{"$nulls":3},"蓄电池安全整改"]
[20,"继电器","RXM4LB1P7 230VAC 5A/250V",null,"个",1,null,null,"施耐德","冷干机更换"]
[21,"剩余电流断路器","HSL1-1004  63A 400V 50HZ ",null,"块",1,null,null,"杭州之江","煤化验更换"]
[22,"热继电器","TA25 DU5 0.5~5 ",null,"个",1,null,null,"ABB","电除尘更换"]
[23,"热继电器","LR2-D1304 N",null,"个",1,null,null,"施耐德","电除尘更换"]
[24,"阴极振打电机","YS7104 0.18KW 380V 0.65A 1440r/min IP55 S1 Y  Φ200mm 轴承6202",null,"台",1,{"$nulls":3},"电除尘更换"]
[25]
[26]
[]
["热工仪表配件类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"电动执行机构伺服电机","DKJ-5100F",null,"台",1,null,null,"天津万方","2#炉引风机执行器"]
[2,"氧传感器","SD-SENSOR-O2",null,"个",1,null,null,"深圳山盾","臭氧氧气泄漏检测仪"]
[3,"磁翻板液位计","UHZ一C13Pa0 L=1400 P=0.6MPa T=80℃ DN20",null,"台",1,{"$nulls":3},"化水碱罐"]
[4,"压力变送器","IGP10-T22E1F-M1L1 0-6Mpa HART",null,"台",1,{"$nulls":3},"锅炉汽水压力"]
[5,"压力变送器","AO3051DPA22AFEB3C2  丁字螺纹接头M20*1.5 -500-500Pa HART",null,"台",1,{"$nulls":3},"膛炉风压"]
[6,"流量二次表","DY21LLB6626AP4M特",null,"台",1,{"$nulls":3},"外管流量计"]
[7,"全功能款手持通讯器","中文版HART475手操器",null,"台",1,null,null,"罗斯蒙特","工具（固定资产）"]
[8,"测速传感器","OVW2-06-2MHT",null,"个",1,null,null,"NIDEC NMICON CORP.","锅炉计量给煤机"]
[9,"氧传感器","Oxy-12",null,"个",1,null,null,"雪迪龙","炉外脱硫烟气监测"]
[10,"压力变送器","AO910J22E2RM3GB3 0-2MPa HART",null,"个",1,null,null,"澳泰","双减压力"]
["专业配套设备配件类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"电力专用UPS","PROTEK AHA-104R DC220 工业级 10KVA 工业级 单进单出 单机 输入、输出双隔离 中文LCD显示 报警干接点，RS485 MODBUS规约，机架式8U",null,"台",1,null,null,"普罗太克","主控室逆变屏更换"]
[2,"储能组件","HDZ-70-30 220V∽  150W",null,"套",1,null,null,"ABB","10KV高压开关更换"]
[3,"逆变馈线柜","PROTEK AHA-OUT-10、10路（16A）交流输出馈线回路、1路（63A）盘间联络开关、断路器指示灯、数字显示仪表、屏顶散热、满足现有UPS嵌入式及隔离变安装、800mm*600mm*2200mm、颜色RAL7032",null,"面",1,null,null,"普罗太克","逆变装置安全提升"]
[4,"蓄电池","GFMJ2V420AH",null,"块",1,null,null,"普罗太克","电池组更换"]
[5]
[6]
["阀门、安全阀、流量计、水泵类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"安全阀","A48Y-16C","PN1.6Mpa,DN100mm，流道通径65mm，整定压力1.0Mpa，压力等级1.0-1.3Mpa，适用介质：蒸汽、空气等","台",1,{"$nulls":3},"天然气锅炉分汽缸安全阀更换"]
[2,"蝶阀","型号：D71X-10,阀体HT20;口径DN65",null,"个",1,{"$nulls":3},"炉外脱硫系统阀门备件"]
[3,"截止阀","J41H-25C   DN50 PN25",null,"台",1,{"$nulls":3},"供热管网疏水"]
[4,"疏水器（热动力）","DT35F-16C","PN1.6Mpa,DN25mm，材质：碳钢，适用介质：蒸汽等","台",1,{"$nulls":3},"供热管道更换疏水器"]
[5,"截止阀","J41H-25","PN2.5Mpa,DN25mm，材质：碳钢，适用介质：蒸汽等","台",1,{"$nulls":3},"供热管道疏水装置更换阀门"]
[6,"闸阀","Z41H-100C  DN20 PN100 425℃","锻钢","个",1,{"$nulls":3},"锅炉检修"]
[7]
["化学试剂、器皿及药品类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"氨水","AR（6瓶/箱）",null,"箱",1,{"$nulls":3},"化水加药"]
[2,"小瓷舟","AS3200-F-003",null,"个",1,null,null,"长沙开元","煤化验"]
[3,"点火丝",null,null,"盒",1,null,null,"长沙开元","煤化验"]
[4,"苯甲酸",null,null,"盒",1,null,null,"长沙开元","煤化验"]
[5,"测硫仪送样杆","5E-S3200",null,"根",1,null,null,"长沙开元","煤化验"]
[6,"标煤"," GBW11101q硫份0.46%",null,"瓶",1,{"$nulls":3},"煤化验标定用"]
[7,"标煤 ","GBW11107l硫份0.82%",null,"瓶",1,{"$nulls":3},"煤化验标定用"]
[8,"标煤 ","GBW11105l硫份1.72%",null,"瓶",1,{"$nulls":3},"煤化验标定用"]
[9,"磷酸三钠","纯度98%、25kg",null,"袋",1,{"$nulls":3},"化水加药"]
[10,"吸耳球","中",null,"个",1,{"$nulls":3},"化水加药"]
[11,"乳胶帽",null,null,"个",1,{"$nulls":3},"化水加药"]
[12,"滴定瓶（棕色）","100ml",null,"个",1,{"$nulls":3},"化水加药"]
[13,"毛刷 ","一寸",null,"把",1,{"$nulls":3},"煤化验"]
[14,"EDTA标准液","0.020000 mmol/L 500ml",null,"瓶",1,{"$nulls":3},"化水配药"]
[15]
[16]
["劳保类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"绝缘鞋","15KV",null,"双",1,{"$nulls":3},"按每年工种实际用量。 注：鞋子码数39-1,40-5,41-3,42-4,43-2"]
[2,"雨鞋","8838黑色中筒",null,"双",1,{"$nulls":3},"按每年工种实际用量。 注：鞋子码数39-1,40-5,41-4,42-4,43-2"]
[3,"单胶雨衣",null,null,"件",1]
[4,"高温鞋",null,null,"双",1]
[5,"帆布工作服",null,null,"套",1]
[6,"棉布工作服",null,null,"套",1]
[7,"防毒面具（滤芯）","3200型灰橡胶口罩",null,"个",1]
[8,"防尘滤芯纸","3200型配套",null,"盒",1]
[9,"披肩工作帽",null,null,"个",1]
[10,"袖套",null,null,"付",1]
[11,"纱手套",null,null,"双",1,{"$nulls":3},"每季度用量"]
[12,"布手套",null,null,"双",1]
[13,"防护眼镜",null,null,"个",1]
[14,"防尘眼镜",null,null,"个",1]
[15,"耐酸碱手套",null,null,"双",1]
[16,"长皮手套（焊工手套）",null,null,"双",1]
[17]
["定制产品类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"严禁攀爬翻越护栏","长50cm*宽40cm","铝板","块",1,{"$nulls":3},"增加煤泥沉淀池标识"]
[2,"“当心坠落”警示牌","长40cm*宽50cm","铝板","块",1,{"$nulls":3},"现场标识更新维护"]
[3,"警示标识牌","立杆φ5cm长2.5m，警示牌50cm*40cm","镀锌管立杆，铝板警示牌","套",1,{"$nulls":3},"完善警示标识"]
[4,"警示标识牌","立杆φ5cm长2.5m，警示牌50cm*40cm","镀锌管立杆，铝板警示牌","套",1,{"$nulls":3},"完善警示标识"]
[5]
[6,{"$nulls":7},"定制"]
["燃料、气体类"]
["序号","请购品名","规格型号","材质","单位","数量","单价","总价","制造厂商","用途说明"]
[1,"氧气",null,null,"瓶",1,{"$nulls":3},"化验室、检修用"]
[2,"乙炔",null,null,"瓶",1,{"$nulls":3},"检修用"]
[3,"氩气",null,null,"瓶",1,{"$nulls":3},"检修用"]
[4,"二氧化硫标准气","866mg/m3 SO2  8L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[5,"二氧化硫标准气","44.7ppm SO2   8L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[6,"一氧化氮标准气","671mg/m3 NO  8L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[7,"一氧化氮标准气","44.8ppm NO    8L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[8,"零气标准气","99.999% N2   8L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[9,"二氧化硫标准气","200mg/m3 SO2  4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[10,"二氧化硫标准气","50mg/m3 SO2  4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[11,"二氧化硫标准气","44.7ppm SO2   4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[12,"二氧化硫标准气","27.7ppm SO2   4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[13,"二氧化硫标准气","  12ppm SO2   4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[14,"一氧化氮标准气","200mg/m3 SO2  4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[15,"一氧化氮标准气","50mg/m3 SO2  4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[16,"一氧化氮标准气","44.8ppm NO    4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[17,"一氧化氮标准气","27.1ppm NO    4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[18,"一氧化氮标准气","12.0ppm NO    4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[19,"零气标准气","99.999% N2    4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[20,"二氧化氮标准气","20ppm NO2 4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[21,"氧气标准气","5.98%    4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[22,"氧气标准气","13.0%    4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]
[23,"氧气标准气","22.1%    4L 9.5MPa",null,"瓶",1,null,null,"上海神开气体技术有限公司","烟气监测标准气"]